{"text_format":"2","workbook":"xlsx","n_sheets":1,"sheets":["A"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"A","index":0,"n_rows":642,"n_cols":5,"rows_kept":642,"cut":false,"hidden":false,"merged":[]}
["Code interne","Description français","Description néerlandais","Dimension en mm","Disponible"]
["AHF/126-S           ","ARM. HAUTE 2 PORTES COUL.+ 3 TABL.REGL.                     ","HOGE KAST 2 SCHUIFDEUREN+3 REGELB.TABL.                     ","1200X600H2000                                     ",1]
["AHF/166-S           ","ARM. HAUTE 2 PORTES COUL.+3 TABL.REGL.                      ","HOGE KAST 2 SCHUIFDEUREN+3 REGELB.TABL                      ","1600X600H2000                                     ",1]
["MRB/0600-S          ","ARMOIRE ENTRETIEN MIXTE 1 PORTE TOIT PENTE                  ","                                                            ","600X500H2000                                      ",2]
["MRB/1000-S          ","ARMOIRE ENTRETIEN MIXTE 2 PORTES TOIT PENTE                 ","BORSTELKAST DUBBEL + SLOT                                   ","1000X500H2000                                     ",1]
["AH2/186-S           ","ARMOIRE HAUTE 2 NIV. 4 PORTES COULISSANTES                  ","HOGE KAST 2 NIV. + 4 SCHUIFDEUREN                           ","1800X600H2000                                     ",1]
["AH2/207-S           ","ARMOIRE HAUTE 2 NIV. 4 PORTES COULISSANTES                  ","HOGE KAST 2 NIV. + 4 SCHUIFDEUREN                           ","2000X700H2000                                     ",1]
["L-AH2/166-S         ","ARMOIRE HAUTE 2 NIV. 4 PORTES COULISSANTES 304SB            ","HOGE KAST 2 NIV. + 4 SCHUIFDEUREN 304SB                     ","1600X600H2000                                     ",1]
["AHF/106-S           ","ARMOIRE HAUTE PORTES COUL.+3 TABL.REGL.                     ","HOGE KAST SCHUIFDEUREN+3 REGELB.TABL                        ","1000X600H2000                                     ",1]
["PL/1215G+PLAF/127   ","PL/1215G + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1215G + KAST MET 2 SCHUIFDEUREN                          ","1200X700H840                                      ",-5]
["PL/1215G+PLAF/127-S ","PL/1215G + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1215G + KAST MET 2 SCHUIFDEUREN                          ","1200X700H840                                      ",2]
["PL/1416G+PLAF/147-S ","PL/1416G + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1416G + KAST MET 2 SCHUIFDEUREN                          ","1400X700H840                                      ",2]
["PL/1424D+PLAF/147-S ","PL/1424D + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1424D + KAST MET 2 SCHUIFDEUREN                          ","1400X700H840                                      ",2]
["PL/1424G+PLAF/147-S ","PL/1424G + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1424G + KAST MET 2 SCHUIFDEUREN                          ","1400X700H840                                      ",1]
["PL/1624D+PLAF/107/-S","PL/1624D + ARMOIRE 2 PORTES +  ESP LV                       ","PL/1624D + KAST 2 DEUREN + RUIMTE VOOR VAATWASSER           ","1600X700H840                                      ",1]
["PL/1624D+PLAF/167-S ","PL/1624D + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1624D + KAST MET 2 SCHUIFDEUREN                          ","1600X700H840                                      ",2]
["PL/1624G+PLAF/167-S ","PL/1624G + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1624G + KAST MET 2 SCHUIFDEUREN                          ","1600X700H840                                      ",1]
["PL/1825D+PLAF/187-S ","PL/1825D + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1825D+ KAST MET 2 SCHUIFDEUREN                           ","1800X700H840                                      ",1]
["PL/1825G+PLAF/127/-S","PL/1825G + ARMOIRE 2 PORTES +  ESP LV                       ","PL/1825G + KAST 2 DEUREN + RUIMTE VOOR VAATWASSER           ","1800X700H840                                      ",2]
["PL/1825G+PLAF/187-S ","PL/1825G + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/1825G+ KAST MET 2 SCHUIFDEUREN                           ","1800X700H840                                      ",2]
["PL/2026D+PLAF/207-S ","PL/2026D + ARMOIRE 2 PORTES COULLISSANTES                   ","PL/2026D+ KAST MET 2 SCHUIFDEUREN                           ","2000X700H840                                      ",1]
["TFC/127+BAF-S       ","TABLE ARM.CHAUFF.2 PORTES COULISSANTES+T+BAF                ","WARMHOUDKAST 2 SCHUIFDEUREN + REGELBLAD+BAF                 ","1200X700H880/900                                  ",2]
["TFC/167+BAF-S       ","TABLE ARM.CHAUFF.2 PORTES COULISSANTES+T+BAF                ","WARMHOUDKAST 2 SCHUIFDEUREN + REGELBLAD+BAF                 ","1600X700H880/900                                  ",1]
["TFC/187+BAF-S       ","TABLE ARM.CHAUFF.2 PORTES COULISSANTES+T+BAF                ","WARMHOUDKAST 2 SCHUIFDEUREN + REGELBLAD+BAF                 ","1800X700H880/900                                  ",1]
["TFC/207+BAF-S       ","TABLE ARM.CHAUFF.2 PORTES COULISSANTES+T+BAF                ","WARMHOUDKAST 2 SCHUIFDEUREN + REGELBLAD+BAF                 ","2000X700H880/900                                  ",1]
["TFC/187-S           ","TABLE ARM.CHAUFF.ECO.2 PORTES COULISS.+T                    ","ECO. WARMHOUDKAST 2 SCHUIFDEUREN+REGELBL                    ","1800X700H880/900                                  ",2]
["TFP/167-S           ","TABLE ARM.PASSANTE 2X2 PORTES COULISS                       ","DOORSCHUIFKAST 2X2 DEUREN VOOR+ACHTER                       ","1600X700H880/900                                  ",2]
["TFP/207-S           ","TABLE ARM.PASSANTE 2X2 PORTES COULISS                       ","DOORSCHUIFKAST 2X2 DEUREN VOOR+ACHTER                       ","2000X700H880/900                                  ",1]
["L-TFTR1/067+BAF-S   ","TABLE ARMOIRE + 1 BLOC DE 3 TIROIRS + BAF AISI304SB         ","TAFELKAST + 1 BLOK VAN 3 LADEN + BAF AISI304SB              ","600X700H880/900                                   ",1]
["TFTR2/107+BAF-S     ","TABLE ARMOIRE + 2 BLOCS DE 3 TIROIRS                        ","TAFELKAST + 2 BLOKKEN VAN 3 LADEN                           ","1000X700H880/900                                  ",1]
["TFTR2/107-S         ","TABLE ARMOIRE + 2 BLOCS DE 3 TIROIRS                        ","TAFELKAST + 2 BLOKKEN VAN 3 LADEN                           ","1000X700H880/900                                  ",1]
["L-TFTR2/107+BAF-S   ","TABLE ARMOIRE + 2 BLOCS DE 3 TIROIRS + BAF AISI304SB        ","TAFELKAST + 2 BLOKKEN VAN 3 LADEN + BAF AISI304SB           ","1000X700H880/900                                  ",1]
["L-TFB/087-S         ","TABLE ARMOIRE 2 PORTE BATTANTE + TI REGL AISI304SB          ","TAFELKAST 2 DRAAIDEUR + REGELB. TABLET AISI304SB            ","800X700H880/900                                   ",3]
["TFB/086-S           ","TABLE ARMOIRE 2 PORTES BATTANTES + TI RE                    ","TAFELKAST 2 DRAAIDEUREN + REGELBAAR TUSS                    ","800X600H880/900                                   ",1]
["TFB/087-S           ","TABLE ARMOIRE 2 PORTES BATTANTES + TI REGL                  ","TAFELKAST 2 DRAAIDEUR + REGELB. TABLET                      ","800X700H880/900                                   ",2]
["TF/106-S            ","TABLE ARMOIRE 2 PORTES COUL.+TI REGLABLE                    ","TAFELKAST 2 SCHUIFDEUREN +REGELB.TABLET                     ","1000X600H880/900                                  ",1]
["TF/106+BAF-S        ","TABLE ARMOIRE 2 PORTES COUL.+TI REGLABLE+BAF                ","TAFELKAST 2 SCHUIFDEUREN +REGELB.TABLET+BAF                 ","1000X600H880/900                                  ",2]
["TF/206-S            ","TABLE ARMOIRE 2 PORTES COULISS.+ TI REGL                    ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","2000X600H880/900                                  ",1]
["TF/147-S            ","TABLE ARMOIRE 2 PORTES COULISSANTES                         ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","1400X700 H880/900                                 ",2]
["TF/167-S            ","TABLE ARMOIRE 2 PORTES COULISSANTES                         ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","1600X700 H880/900                                 ",1]
["TF/187-S            ","TABLE ARMOIRE 2 PORTES COULISSANTES                         ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","1800X700 H880/900                                 ",1]
["TF/207+TS3-S        ","TABLE ARMOIRE 2 PORTES COULISSANTES                         ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","2000X700 H880/900                                 ",2]
["TF/207-S            ","TABLE ARMOIRE 2 PORTES COULISSANTES                         ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","2000X700 H880/900                                 ",1]
["L-TF/167-S          ","TABLE ARMOIRE 2 PORTES COULISSANTES 304SB                   ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET 304SB              ","1600X700 H880/900                                 ",1]
["L-TF/187-S          ","TABLE ARMOIRE 2 PORTES COULISSANTES 304SB                   ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET 304SB              ","1800X700 H880/900                                 ",1]
["L-TF/207-S          ","TABLE ARMOIRE 2 PORTES COULISSANTES 304SB                   ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET 304SB              ","2000X700 H880/900                                 ",1]
["L-TF/207+TS3-S      ","TABLE ARMOIRE 2 PORTES COULISSANTES AISI304SB               ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET AISI304SB          ","2000X700 H880/900                                 ",1]
["TF/126-S            ","TABLE ARMOIRE 2 PORTES COULISSANTES+ TI                     ","TAFELKAST 2 SCHUIFDEUREN +REGELB.TABLET                     ","1200X600H880/900                                  ",1]
["TF/146-S            ","TABLE ARMOIRE 2 PORTES COULISSANTES+ TI                     ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","1400X600H880/900                                  ",1]
["TF/186-S            ","TABLE ARMOIRE 2 PORTES COULISSANTES+ TI                     ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","1800X600H880/900                                  ",2]
["TF/208-S            ","TABLE ARMOIRE 2 PORTES COULISSANTES+ TI                     ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET                    ","2000X800H880/900                                  ",1]
["TF/146+BAF-S        ","TABLE ARMOIRE 2 PORTES COULISSANTES+ TI+BAF                 ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET+BAF                ","1400X600H880/900                                  ",1]
["L-TF/126+BAF-S      ","TABLE ARMOIRE 2 PORTES COULISSANTES+ TI+BAF AISI304SB       ","TAFELKAST 2 SCHUIFDEUREN +REGELB.TABLET+BAF AISI304SB       ","1200X600H880/900                                  ",1]
["TF/107+BAF-S        ","TABLE ARMOIRE 2 PORTES COULISSANTES+BAF                     ","TAFELKAST 2 SCHUIFDEUREN +REGELB.TABLET+BAF                 ","1000X700 H880/900                                 ",2]
["TF/127+BAF-S        ","TABLE ARMOIRE 2 PORTES COULISSANTES+BAF                     ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET+BAF                ","1200X700 H880/900                                 ",5]
["TF/147+BAF-S        ","TABLE ARMOIRE 2 PORTES COULISSANTES+BAF                     ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET+BAF                ","1400X700 H880/900                                 ",1]
["TF/207+BAF-S        ","TABLE ARMOIRE 2 PORTES COULISSANTES+BAF                     ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET+BAF                ","2000X700 H880/900                                 ",3]
["L-TF/127+BAF-S      ","TABLE ARMOIRE 2 PORTES COULISSANTES+BAF 304SB               ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET+BAF 304SB          ","1200X700 H880/900                                 ",1]
["L-TF/187+BAF-S      ","TABLE ARMOIRE 2 PORTES COULISSANTES+BAF 304SB               ","TAFELKAST 2 SCHUIFDEUREN +REGELB. TABLET+BAF 304SB          ","1800X700 H880/900                                 ",1]
["L-TFBA-700+BAF-S    ","TABLE ARMOIRE ANGULAIRE PORTE BAT+BAF AISI304               ","HOEKTAFELKAST MET DRAAIDEUR+BAF AISI304                     ","1000X1000X700H880/900                             ",1]
["TAO/208-S           ","TABLE ARMOIRE OUVERTE AVEC TABLETTE REGL                    ","OPEN TAFELKAST MET REGELBAAR TUSSENBLAD                     ","2000X800H880/900                                  ",2]
["ASF/124-S           ","ARMOIRE SUSPENDUE 2 PORTES COULISSANTES                     ","GESLOTEN HANGKAST MET 2 SCHUIFDEUREN                        ","1200X400H600                                      ",1]
["ASF/144-S           ","ARMOIRE SUSPENDUE 2 PORTES COULISSANTES                     ","GESLOTEN HANGKAST MET 2 SCHUIFDEUREN                        ","1400X400H600                                      ",4]
["ASF/204-S           ","ARMOIRE SUSPENDUE 2 PORTES COULISSANTES                     ","GESLOTEN HANGKAST MET 2 SCHUIFDEUREN                        ","2000X400H600                                      ",6]
["L-ASF/124-S         ","ARMOIRE SUSPENDUE 2 PORTES COULISSANTES 304SB               ","GESLOTEN HANGKAST MET 2 SCHUIFDEUREN 304SB                  ","1200X400H600                                      ",1]
["L-ASF/184-S         ","ARMOIRE SUSPENDUE 2 PORTES COULISSANTES 304SB               ","GESLOTEN HANGKAST MET 2 SCHUIFDEUREN 304SB                  ","1800X400H600                                      ",2]
["L-AST/1800-S        ","TOIT INCLINE POUR ARMOIRE SUSPENDUE 1800 AISI304SB          ","                                                            ","1800X400H170                                      ",5]
["CS/50-S             ","CAISSON ISOLE EN GALVA POUR VENTILATEUR                     ","GEISOLEERDE GALVA KIST VOOR VENTILATOR                      ","500X500XH500                                      ",2]
["CS/60-S             ","CAISSON ISOLE EN GALVA POUR VENTILATEUR                     ","GEISOLEERDE GALVA KIST VOOR VENTILATOR                      ","600X600XH600                                      ",2]
["CSL/50-S            ","CAISSON LUXE ISOLE EN GALVA POUR VENTILA                    ","GEISOLEERDE LUXE GALVA KIST VOOR VENTILA                    ","500X500XH500                                      ",2]
["CC50-S              ","CONSOLES POUR CAISSON 500                                   ","STEUNEN VOOR KIST 500                                       ","                                                  ",2]
["CC60/70-S           ","CONSOLES POUR CAISSON 600 & 700                             ","STEUNEN VOOR KIST 600 & 700                                 ","600/700                                           ",18]
["ST/3-S              ","AVALOIR INOX + GRILLE/30                                    ","INOX STERFPUT + ROOSTER/30                                  ","300X300xh130                                      ",4]
["ST-CNL-CNC/CLOCHE-S ","CLOCHE POUR STERPUT ET CANIVEAUX                            ","REUKKLOK VOOR STERPUTTEN EN GRONDROOSTERS                   ","Ø130 H50                                          ",7]
["CM3A-S              ","CHAUFFE-METS RESISTANCE INOX 1250W/230V                     ","RVS WARMTESTRALER 1250 W / 230 V                            ","1260X150XH60                                      ",-3]
["CM4A-S              ","CHAUFFE-METS RESISTANCE INOX 1600W/230V                     ","RVS WARMTESTRALER 1600W/230V                                ","1560X150XH60                                      ",-3]
["CM5A-S              ","CHAUFFE-METS RESISTANCE INOX 2000W/230V                     ","RVS WARMTESTRALER 2000 W / 230 V                            ","1960X150XH60                                      ",-1]
["CM2A-S              ","CHAUFFE-METS RESISTANCE INOX 800W/230V                      ","RVS WARMTESTRALER 800 W / 230 V                             ","860X150XH60                                       ",-6]
["CMKIT-S-C           ","KIT DE 2 PIEDS POUR CHAUFFE-METS                            ","ONDERSTEL VOOR WARMTESTRALER                                ","Ø14 H400                                          ",3]
["PLDS/0715+PP/0-S    ","PLONGE EN KIT 1 CUVE                                        ","SPOELTAFEL KIT 1 BAK                                        ","700X700H900                                       ",1]
["PLDS/60615+PP/0-S   ","PLONGE EN KIT 1 CUVE                                        ","SPOELTAFEL KIT 1 BAK                                        ","600X600H900                                       ",1]
["PLDS/1416D+PP/0-S   ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR DROITE                     ","SPOELTAFEL KIT 1 BAK + AFDRUIP RECHTS                       ","1400X700H900                                      ",1]
["PLDS/61014D+PP/0-S  ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR DROITE                     ","SPOELTAFEL KIT 1 BAK + AFDRUIP RECHTS                       ","1000X600H900                                      ",2]
["PLDS/1416D+P0/LV-S  ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR DX + ESP LV                ","SPOELTAFEL KIT 1 BAK + AFDRUIP R + ESP LV                   ","1400X700H900                                      ",5]
["PLDS/61215D+P0/LV-S ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR DX + ESP LV                ","SPOELTAFEL KIT 1 BAK + AFDRUIP R + ESP LV                   ","1200X600H900                                      ",1]
["PLDS/1215D+P0/LV-S  ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR DX+ESP LV                  ","SPOELTAFEL KIT 1 BAK + AFDRUIP R + ESP LV                   ","1200X700H900                                      ",6]
["PLDS/1215G+PP/0-S   ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR GAUCHE                     ","SPOELTAFEL KIT 1 BAK + AFDRUIP LINKS                        ","1200X700H900                                      ",2]
["PLDS/61014G+PP/0-S  ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR GAUCHE                     ","SPOELTAFEL KIT 1 BAK + AFDRUIP LINKS                        ","1000X600H900                                      ",2]
["PLDS/1416G+P0/LV-S  ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR GX + ESP LV                ","SPOELTAFEL KIT 1 BAK + AFDRUIP L + ESP LV                   ","1400X700H900                                      ",3]
["PLDS/1215G+P0/LV-S  ","PLONGE EN KIT 1 CUVE+1 EGOUTTOIR GX+ESP LV                  ","SPOELTAFEL KIT 1 BAK + AFDRUIP L + ESP LV                   ","1200X700H900                                      ",6]
["PLDS/1424D+PP/0-S   ","PLONGE EN KIT 2 CUVES+1 EGOUTTOIR DROITE                    ","SPOELTAFEL KIT 2 BAKKEN+ AFDRUIP RECHTS                     ","1400X700H900                                      ",1]
["PLDS/1624D+PP/0-S   ","PLONGE EN KIT 2 CUVES+1 EGOUTTOIR DROITE                    ","SPOELTAFEL KIT 2 BAKKEN + AFDRUIP RECHTS                    ","1600X700H900                                      ",2]
["PLDS/1825D+PP/0-S   ","PLONGE EN KIT 2 CUVES+1 EGOUTTOIR DROITE                    ","SPOELTAFEL KIT 2 BAKKEN + AFDRUIP RECHTS                    ","1800X700H900                                      ",2]
["PLDS/2026D+PP/0-S   ","PLONGE EN KIT 2 CUVES+1 EGOUTTOIR DROITE                    ","SPOELTAFEL KIT 2 BAKKEN + AFDRUIP RECHTS                    ","2000X700H900                                      ",1]
["PLDS/1624D+P0/LV-S  ","PLONGE EN KIT 2 CUVES+1 EGOUTTOIR DX + ESP LV               ","SPOELTAFEL KIT 2 BAKKEN + AFDRUIP R + ESP LV                ","1600X700H900                                      ",2]
["PLDS/1624G+PP/0-S   ","PLONGE EN KIT 2 CUVES+1 EGOUTTOIR GAUCHE                    ","SPOELTAFEL KIT 2 BAKKEN + AFDRUIP LINKS                     ","1600X700H900                                      ",2]
["PLDS/1825G+PP/0-S   ","PLONGE EN KIT 2 CUVES+1 EGOUTTOIR GAUCHE                    ","SPOELTAFEL KIT 2 BAKKEN + AFDRUIP LINKS                     ","1800X700H900                                      ",2]
["PLDS/61424G+PP/0-S  ","PLONGE EN KIT 2 CUVES+1 EGOUTTOIR GAUCHE                    ","SPOELTAFEL KIT 2 BAKKEN + AFDRUIP LINKS                     ","1400X600H900                                      ",2]
["PLDS/2025+PP/0-S    ","PLONGE EN KIT 2 CUVES+2 EGOUTTOIRS                          ","SPOELTAFEL KIT 2 BAKKEN + 2 AFDRUIPEN                       ","2000X700H900                                      ",2]
["TTDS/0661-S         ","TABLE EN KIT   600X600                                      ","DEMONTEERBARE TAFEL 600X600                                 ","600X600H900                                       ",1]
["TTDSB0/0770-S       ","TABLE EN KIT   700X700 + BAF SANS SOUS-TABLETTE             ","DEMONTEERBARE TAFEL 700X700 + BAF                           ","700X700H900                                       ",4]
["TTDS0/0770-S        ","TABLE EN KIT   700X700 SANS SOUS-TABLETTE                   ","DEMONTEERBARE TAFEL 700X700 ZONDER ONDERTABLET              ","700X700H900                                       ",4]
["TTDS/0871-S         ","TABLE EN KIT   800X700                                      ","DEMONTEERBARE TAFEL 800X700                                 ","800X700H900                                       ",1]
["TTDSB/0871-S        ","TABLE EN KIT   800X700 + BAF                                ","DEMONTEERBARE TAFEL 800X700 + BAF                           ","800X700H900                                       ",1]
["TTDSB0/0870-S       ","TABLE EN KIT   800X700 + BAF SANS SOUS-TABLETTE             ","DEMONTEERBARE TAFEL 800X700 + BAF                           ","800X700H900                                       ",4]
["TTDS/0971-S         ","TABLE EN KIT   900X700                                      ","DEMONTEERBARE TAFEL 900X700                                 ","900X700H900                                       ",4]
["TTDSB0/1070-S       ","TABLE EN KIT 1000X700 + BAF SANS SOUS-TABLETTE              ","DEMONTEERBARE TAFEL 1000X700 + BAF                          ","1000X700H900                                      ",3]
["TTDS0/1070-S        ","TABLE EN KIT 1000X700 SANS SOUS-TABLETTE                    ","DEMONTEERBARE TAFEL 1000X700 ZONDER ONDERTABLET             ","1000X700H900                                      ",4]
["TTDS/1261-S         ","TABLE EN KIT 1200X600                                       ","DEMONTEERBARE TAFEL 1200X600                                ","1200X600H900                                      ",5]
["TTDSB/1261-S        ","TABLE EN KIT 1200X600 + BAF                                 ","DEMONTEERBARE TAFEL 1200X600 + BAF                          ","1200X600H900                                      ",2]
["TTDS/1271-S         ","TABLE EN KIT 1200X700                                       ","DEMONTEERBARE TAFEL 1200X700                                ","1200X700H900                                      ",1]
["TTDSB/1271-S        ","TABLE EN KIT 1200X700 + BAF                                 ","DEMONTEERBARE TAFEL 1200X700 + BAF                          ","1200X700H900                                      ",1]
["TTDS0/1270-S        ","TABLE EN KIT 1200X700 SANS SOUS-TABLETTE                    ","DEMONTEERBARE TAFEL 1200X700 ZONDER ONDERTABLET             ","1200X700H900                                      ",4]
["TTDS/1461-S         ","TABLE EN KIT 1400X600                                       ","DEMONTEERBARE TAFEL 1400X600                                ","1400X600H900                                      ",2]
["TTDSB/1461-S        ","TABLE EN KIT 1400X600 + BAF                                 ","DEMONTEERBARE TAFEL 1400X600 + BAF                          ","1400X600H900                                      ",1]
["TTDSB/1471-S        ","TABLE EN KIT 1400X700 + BAF                                 ","DEMONTEERBARE TAFEL 1400X700 + BAF                          ","1400X700H900                                      ",4]
["TTDSB0/1470-S       ","TABLE EN KIT 1400X700 + BAF SANS SOUS-TABLETTE              ","DEMONTEERBARE TAFEL 1400X700 + BAF                          ","1400X700H900                                      ",3]
["TTDS/1661-S         ","TABLE EN KIT 1600X600                                       ","DEMONTEERBARE TAFEL 1600X600                                ","1600X600H900                                      ",2]
["TTDSB/1661-S        ","TABLE EN KIT 1600X600 + BAF                                 ","DEMONTEERBARE TAFEL 1600X600 + BAF                          ","1600X600H900                                      ",2]
["TTDS/1671-S         ","TABLE EN KIT 1600X700                                       ","DEMONTEERBARE TAFEL 1600X700                                ","1600X700H900                                      ",1]
["TTDSB/1671-S        ","TABLE EN KIT 1600X700 + BAF                                 ","DEMONTEERBARE TAFEL 1600X700 + BAF                          ","1600X700H900                                      ",6]
["TTDSB0/1670-S       ","TABLE EN KIT 1600X700 + BAF SANS SOUS-TABLETTE              ","DEMONTEERBARE TAFEL 1600X700 + BAF                          ","1600X700H900                                      ",3]
["TTDS0/1670-S        ","TABLE EN KIT 1600X700 SANS SOUS-TABLETTE                    ","DEMONTEERBARE TAFEL 1600X700 ZONDER ONDERTABLET             ","1600X700H900                                      ",1]
["TTDS/1861-S         ","TABLE EN KIT 1800X600                                       ","DEMONTEERBARE TAFEL 1800X600                                ","1800X600H900                                      ",2]
["TTDSB/1871-S        ","TABLE EN KIT 1800X700 + BAF                                 ","DEMONTEERBARE TAFEL 1800X700 + BAF                          ","1800X700H900                                      ",2]
["TTDSB0/1870-S       ","TABLE EN KIT 1800X700 + BAF SANS SOUS-TABLETTE              ","DEMONTEERBARE TAFEL 1800X700 + BAF                          ","1800X700H900                                      ",3]
["TTDS0/1870-S        ","TABLE EN KIT 1800X700 SANS SOUS-TABLETTE                    ","DEMONTEERBARE TAFEL 1800X700                                ","1800X700H900                                      ",4]
["TTDS/2061-S         ","TABLE EN KIT 2000X600                                       ","DEMONTEERBARE TAFEL 2000X600                                ","2000X600H900                                      ",3]
["TTDSB/2071-S        ","TABLE EN KIT 2000X700 + BAF                                 ","DEMONTEERBARE TAFEL 2000X700 + BAF                          ","2000X700H900                                      ",1]
["TTDSB0/2070-S       ","TABLE EN KIT 2000X700 + BAF SANS SOUS-TABLETTE              ","DEMONTEERBARE TAFEL 2000X700 + BAF                          ","2000X700H900                                      ",2]
["DSTI/1070-S         ","TABLETTE INFERIEUR DEM 1000X700                             ","                                                            ","1000X700H150                                      ",4]
["DSTI/1260-S         ","TABLETTE INFERIEUR DEM 1200X600                             ","                                                            ","1200X600XH150                                     ",3]
["DSTI/1470-S         ","TABLETTE INFERIEUR DEM 1400X700                             ","                                                            ","1400X700H150                                      ",1]
["DSTI/1870-S         ","TABLETTE INFERIEUR DEM 1800X700                             ","                                                            ","1800X700XH150                                     ",5]
["DSTI/0660-S         ","TABLETTE INFERIEUR DEM 600X600                              ","                                                            ","600X600XH150                                      ",4]
["PLDSTI/0660-S       ","TABLETTE INFERIEUR PLDS   600X600                           ","ONDERTABLET PLDS 600X600                                    ","600X600H150                                       ",2]
["PLDSTI/0670-S       ","TABLETTE INFERIEUR PLDS   600X700                           ","ONDERTABLET PLDS 600X700                                    ","600X700H150                                       ",2]
["PLDSTI/0870-S       ","TABLETTE INFERIEUR PLDS   800X700                           ","ONDERTABLET PLDS 800X700                                    ","800X700H150                                       ",2]
["PLDSTI/1270-S       ","TABLETTE INFERIEUR PLDS 1200X700                            ","ONDERTABLET PLDS 1200X600                                   ","1200X700H150                                      ",5]
["PLDSTI/1460-S       ","TABLETTE INFERIEUR PLDS 1400X600                            ","ONDERTABLET PLDS 1400X600                                   ","1400X600H150                                      ",1]
["PLDSTI/1470-S       ","TABLETTE INFERIEUR PLDS 1400X700                            ","ONDERTABLET PLDS 1400X600                                   ","1400X700H150                                      ",3]
["PLDSTI/1670-S       ","TABLETTE INFERIEUR PLDS 1600X700                            ","ONDERTABLET PLDS 1600X700                                   ","1600X700H150                                      ",1]
["PLDSTI/1870-S       ","TABLETTE INFERIEUR PLDS 1800X700                            ","ONDERTABLET PLDS 1800X700                                   ","1800X700H150                                      ",1]
["PLDSTI/2070-S       ","TABLETTE INFERIEUR PLDS 2000X700                            ","ONDERTABLET PLDS 2000X700                                   ","2000X700H150                                      ",1]
["LV(S)-1600GX+TI-S   ","SORTIE LAVE VAISSELLE 1600 + SOUS-TABLET                    ","UITLOOPTAFEL 1600 + ONDERBLAD                               ","1600X700H880                                      ",1]
["ECL/CM4A-2NIV-S     ","ETAGERE CHAUFFANTE 2 NIVEAUX                                ","WARMHOUDBRUG 2 NIVEAUS                                      ","1600X300XH700                                     ",-3]
["ECL/CM5A-2NIV-S     ","ETAGERE CHAUFFANTE 2 NIVEAUX                                ","WARMHOUDBRUG 2 NIVEAUS                                      ","2000X300XH700                                     ",-2]
["ECL/10302-S         ","ETAGERE CHEF LISSE 2 NIVEAUX                                ","VLAK CHEFREK 2 NIVEAUS                                      ","1000X300H700                                      ",2]
["ECL/11402-S         ","ETAGERE CHEF LISSE 2 NIVEAUX                                ","VLAK CHEFREK 2 NIVEAUS                                      ","1100X400H700                                      ",1]
["ECL/13252-S         ","ETAGERE CHEF LISSE 2 NIVEAUX                                ","VLAK CHEFREK 2 NIVEAUS                                      ","1300X250H700                                      ",1]
["ECL/14302-S         ","ETAGERE CHEF LISSE 2 NIVEAUX                                ","VLAK CHEFREK 2 NIVEAUS                                      ","1400X300H700                                      ",3]
["ECL/16302-S         ","ETAGERE CHEF LISSE 2 NIVEAUX                                ","VLAK CHEFREK 2 NIVEAUS                                      ","1600X300H700                                      ",3]
["ECL/18302-S         ","ETAGERE CHEF LISSE 2 NIVEAUX                                ","VLAK CHEFREK 2 NIVEAUS                                      ","1800X300H700                                      ",4]
["ECL/20302-S         ","ETAGERE CHEF LISSE 2 NIVEAUX                                ","VLAK CHEFREK 2 NIVEAUS                                      ","2000X300H700                                      ",4]
["ECL/14303-S         ","ETAGERE CHEF LISSE 3 NIVEAUX                                ","VLAK CHEFREK 3 NIVEAUS                                      ","1400X300H900                                      ",1]
["CRA/250-S           ","CONSOLE POUR ETAGERE AJOUREE REGLABLE                       ","STEUN VOOR REGELBAAR OPENGEWERKT MUURREK                    ","250                                               ",5]
["CRA/300-S           ","CONSOLE POUR ETAGERE AJOUREE REGLABLE                       ","STEUN VOOR REGELBAAR OPENGEWERKT MUURREK                    ","300                                               ",16]
["CRA/350-S           ","CONSOLE POUR ETAGERE AJOUREE REGLABLE                       ","STEUN VOOR REGELBAAR OPENGEWERKT MUURREK                    ","350                                               ",36]
["CRA/400-S           ","CONSOLE POUR ETAGERE AJOUREE REGLABLE                       ","STEUN VOOR REGELBAAR OPENGEWERKT MUURREK                    ","400                                               ",8]
["CRA/500-S           ","CONSOLE POUR ETAGERE AJOUREE REGLABLE                       ","STEUN VOOR REGELBAAR OPENGEWERKT MUURREK                    ","500                                               ",21]
["CR/200-S            ","CONSOLE POUR ETAGERE MURALE REGLABLE                        ","STEUN VOOR REGELBAAR MUURREK                                ","200                                               ",25]
["CR/250-S            ","CONSOLE POUR ETAGERE MURALE REGLABLE                        ","STEUN VOOR REGELBAAR MUURREK                                ","250                                               ",18]
["CR/300-S            ","CONSOLE POUR ETAGERE MURALE REGLABLE                        ","STEUN VOOR REGELBAAR MUURREK                                ","300                                               ",-149]
["CR/450-S            ","CONSOLE POUR ETAGERE MURALE REGLABLE                        ","STEUN VOOR REGELBAAR MUURREK                                ","450                                               ",53]
["CR/500-S            ","CONSOLE POUR ETAGERE MURALE REGLABLE                        ","STEUN VOOR REGELBAAR MUURREK                                ","500                                               ",27]
["CR/400-S            ","CONSOLE POUR ETAGERE MURALE REGLABLE  .                     ","STEUN VOOR REGELBAAR MUURREK                                ","400                                               ",-27]
["LE/330-S            ","LATTE POUR ETAGERE MURALE REGLABLE 1 NIV                    ","LAT VOOR REGELBAAR MUURREK 1 NIV.                           ","330                                               ",126]
["LE/660-S            ","LATTE POUR ETAGERE MURALE REGLABLE 2 NIV                    ","LAT VOOR REGELBAAR MUURREK 2 NIV.                           ","660X80                                            ",-36]
["LE/990-S            ","LATTE POUR ETAGERE MURALE REGLABLE 3 NIV                    ","LAT VOOR REGELBAAR MUURREK 3 NIV.                           ","990                                               ",42]
["CFAN/251-S          ","NOUVELLE CONSOLE FIX AJOUREE 250                            ","NIEUWE VASTE CONSOLE VOOR OPENGEWERKT MUURREK 250           ","250                                               ",39]
["CFAN/301-S          ","NOUVELLE CONSOLE FIX AJOUREE 300                            ","NIEUWE VASTE CONSOLE VOOR OPENGEWERKT MUURREK 300           ","300                                               ",-2]
["CFAN/351-S          ","NOUVELLE CONSOLE FIX AJOUREE 350                            ","NIEUWE VASTE CONSOLE VOOR OPENGEWERKT MUURREK 350           ","350                                               ",106]
["CFAN/401-S          ","NOUVELLE CONSOLE FIX AJOUREE 400                            ","NIEUWE VASTE CONSOLE VOOR OPENGEWERKT MUURREK 400           ","400                                               ",7]
["CFAN/501-S          ","NOUVELLE CONSOLE FIX AJOUREE 500                            ","NIEUWE VASTE CONSOLE VOOR OPENGEWERKT MUURREK 500           ","500                                               ",12]
["CFN/201-S           ","NOUVELLE CONSOLE FIXE 200                                   ","NIEUWE VASTE CONSOLE 200                                    ","200                                               ",18]
["CFN/251-S           ","NOUVELLE CONSOLE FIXE 250                                   ","NIEUWE VASTE CONSOLE 250                                    ","250                                               ",-9]
["CFN/301-S           ","NOUVELLE CONSOLE FIXE 300                                   ","NIEUWE VASTE CONSOLE 300                                    ","300                                               ",-29]
["CFN/351-S           ","NOUVELLE CONSOLE FIXE 350                                   ","NIEUWE VASTE CONSOLE 350                                    ","350                                               ",14]
["CFN/401-S           ","NOUVELLE CONSOLE FIXE 400                                   ","NIEUWE VASTE CONSOLE 400                                    ","400                                               ",-39]
["CFN/501-S           ","NOUVELLE CONSOLE FIXE 500                                   ","NIEUWE VASTE CONSOLE 500                                    ","500                                               ",9]
["EDSL/12404-S        ","ETAGERE DE SOL LISSE 4 NIVEAUX                              ","VLAK STAAND REK 4 NIVEAUS                                   ","1200X400H1800                                     ",3]
["EDSL/13404-S        ","ETAGERE DE SOL LISSE 4 NIVEAUX                              ","VLAK STAAND REK 4 NIVEAUS                                   ","1300X400H1800                                     ",1]
["EDSL/14404          ","ETAGERE DE SOL LISSE 4 NIVEAUX                              ","VLAK STAAND REK 4 NIVEAUS                                   ","1400X400H1800                                     ",-1]
["EDSL/16404-S        ","ETAGERE DE SOL LISSE 4 NIVEAUX                              ","VLAK STAAND REK 4 NIVEAUS                                   ","1600X400H1800                                     ",2]
["EDSL/19404-S        ","ETAGERE DE SOL LISSE 4 NIVEAUX                              ","VLAK STAAND REK 4 NIVEAUS                                   ","1900X400H1800                                     ",1]
["EDSL/19504-S        ","ETAGERE DE SOL LISSE 4 NIVEAUX                              ","VLAK STAAND REK 4 NIVEAUS                                   ","1900X500H1800                                     ",3]
["EDSL/20404-S        ","ETAGERE DE SOL LISSE 4 NIVEAUX                              ","VLAK STAAND REK 4 NIVEAUS                                   ","2000X400H1800                                     ",1]
["EMA/1125-S          ","ETAGERE MURALE AJOUREE                                      ","OPENGEWERKT MUURREK                                         ","1100X250                                          ",2]
["EML/0630-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","600X300                                           ",5]
["EML/0635-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","600X350                                           ",4]
["EML/0640-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","600X400                                           ",-4]
["EML/0730-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","700X300                                           ",3]
["EML/0740-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","700X400                                           ",2]
["EML/0830-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","800X300                                           ",-7]
["EML/0840-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","800X400                                           ",3]
["EML/0930-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","900X300                                           ",-1]
["EML/1030-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1000X300                                          ",-22]
["EML/1040-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1000X400                                          ",-16]
["EML/1130-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1100X300                                          ",5]
["EML/1140-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1100X400                                          ",1]
["EML/1230-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1200X300                                          ",-15]
["EML/1240-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1200X400                                          ",-8]
["EML/1330-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1300X300                                          ",-4]
["EML/1350-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1300X500                                          ",10]
["EML/1430-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1400X300                                          ",-6]
["EML/1440-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1400X400                                          ",-22]
["EML/1450-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1400X500                                          ",12]
["EML/1630-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1600X300H30                                       ",20]
["EML/1640-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1600X400                                          ",7]
["EML/1725-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1700X250                                          ",1]
["EML/1730-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1700X300                                          ",1]
["EML/1740-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1700X400                                          ",1]
["EML/1830-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1800X300                                          ",-11]
["EML/1840-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1800X400                                          ",3]
["EML/1940-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","1900X400                                          ",2]
["EML/2030-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","2000X300H30                                       ",-21]
["EML/2040-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","2000X400                                          ",-18]
["EML/2225-S          ","ETAGERE MURALE LISSE                                        ","VLAK MUURREK                                                ","2200X250                                          ",1]
["ASIA1/C1L-S         ","CUISINIERE  ASIA1 (1 GRAND BRÛLEUR)                         ","FORNUIS ASIA 1 (1 GROTE BRANDER)                            ","600 X 630 X 760H                                  ",3]
["ASIA1/C2L-S         ","CUISINIERE  ASIA1 (2 GRANDS BRÛLEURS)                       ","FORNUIS ASIA 1 (2 GROTE BRANDERS)                           ","1200X630H760                                      ",1]
["ASIA1/C3L-S         ","CUISINIERE  ASIA1 (3 GRANDS BRÛLEURS)                       ","FORNUIS ASIA 1 (3 GROTE BRANDERS)                           ","1500X630H760                                      ",-1]
["ASIA2/C3R11-S       ","CUISINIERE ASIA2 3 BRÛLEURS (2GD+1PT)                       ","FORNUIS ASIA 2 3 BRANDERS (2GR+1KL)                         ","1100X900X760/1300                                 ",-2]
["ASIA2/C3R14-S       ","CUISINIERE ASIA2 3 BRÛLEURS (2GD+1PT)                       ","FORNUIS ASIA 2 3 BRANDERS (2GR+1KL)                         ","1400X900X760/1300                                 ",2]
["ASIA2/C5R-S         ","CUISINIERE ASIA2 5 BRÛLEURS  (3GD+2PT)                      ","FORNUIS ASIA 2 5 BRANDERS (3GR+2KL)                         ","1800X900X760/1300H                                ",1]
["W/RDC3R11-S         ","RIDEAU D'EAU C3R/1.1 FINI (SOUDEUR)                         ","                                                            ","1093X625                                          ",5]
["W/RDC5R-S           ","RIDEAU D'EAU C5R+JUMBO+C4R+C3F FINI COMP. EXT               ","                                                            ","1788X625                                          ",1]
["W/TOPC1L-CLP-S      ","TOP C1L + CLP FINI (SOUDEUR)                                ","                                                            ","                                                  ",6]
["W/TOPC2L-S          ","TOP C2L-CLP2 FINI (SOUDEUR)                                 ","                                                            ","1400.4X788.28                                     ",6]
["W/TOPC3L-S          ","TOP C3L (SOUDEUR)                                           ","                                                            ","1700.4X788.28                                     ",2]
["W/TOPC3R11-S        ","TOP C3R/1.1 (SOUDURE)                                       ","                                                            ","1233.6X988.28                                     ",1]
["F/BACFR1POT-MECA-S  ","BAC A FRITES 1 POT   MECA FINI                              ","FRIETENBAK 1 POT MECA AFGEWERKT                             ","                                                  ",6]
["F/BACFR2POT-MECA-S  ","BAC A FRITES 2 POTS MECA FINI                               ","FRIETENBAK 2 POT MECA AFGEWERKT                             ","                                                  ",-1]
["F/BACFR3POT-MECA-S  ","BAC A FRITES 3 POTS MECA FINI                               ","FRIETENBAK 3 POT MECA AFGEWERKT                             ","                                                  ",2]
["F/BACRECUP-S        ","BAC DE RECUPERATION POUR FRITEUSES FINI                     ","OPVANGBAK FRITEUSE AFGEWERKT                                ","                                                  ",4]
["F/CHEMINEE-S        ","CHEMINEE FRITEUSE FINI                                      ","SCHOUW FRITEUSE                                             ","                                                  ",9]
["F/COUVERCLE-DIA-S   ","COUVERCLE  FRITEUSE DIAMOND                                 ","                                                            ","                                                  ",5]
["F/COUVERCLE-S       ","COUVERCLE  FRITEUSE FINI                                    ","DEKSEL FRITEUSE                                             ","                                                  ",7]
["F/FA-1POT-MECA-S    ","FACE AVANT FRITEUSE 1 POT FINI                              ","VOORPANEEL FRITEUSE 1 BAK                                   ","                                                  ",5]
["F/FA-2POT-MECA-S    ","FACE AVANT FRITEUSE 2 POTS FINI                             ","VOORPANEEL FRITEUSE 2 BAKKEN                                ","                                                  ",-4]
["F/FILTREPOT-S       ","FILTRES POUR POT FRITEUSE FINI                              ","FILTER VOOR BAK FRITEUSE                                    ","Ø65/90 X H75                                      ",4]
["F/PORTE1P-S         ","PORTES FRITEUSE 1 POT FINI                                  ","                                                            ","                                                  ",12]
["F/PORTE2&3P-S       ","PORTES FRITEUSE 2&3 POTS FINI                               ","                                                            ","                                                  ",-6]
["F/POT-S             ","POT FRITEUSE FINI                                           ","BAK VOOR FRITEUSE                                           ","                                                  ",-9]
["F/TOP-1POT-S        ","TOP FRITEUSE 1POT FINI                                      ","TOP VOOR FRITEUSE 1 BAK                                     ","                                                  ",4]
["F/TOP-2POT-S        ","TOP FRITEUSE 2POTS FINI                                     ","TOP VOOR FRITEUSE 2 BAKKEN                                  ","                                                  ",6]
["F/TOP-3POT-S        ","TOP FRITEUSE 3POTS FINI                                     ","TOP VOOR FRITEUSE 3 BAKKEN                                  ","                                                  ",5]
["ELECTRO-FRYER 2B-S  ","FRITEUSE ELECTRONIQUE BERTRAND 2 POTS                       ","                                                            ","1140x1000x880/1490                                ",2]
["ELECTRO-FRYER 3B-S  ","FRITEUSE ELECTRONIQUE BERTRAND 3 POTS                       ","                                                            ","1650x1000x880/1490                                ",1]
["MECA-FRYER 1B-S     ","FRITEUSE MECANIQUE BERTRAND 1 POT                           ","MECANISCHE FRITEUSE 1 KUIP                                  ","540X890XH930/1290                                 ",1]
["MECA-FRYER 2B-S     ","FRITEUSE MECANIQUE BERTRAND 2 POTS                          ","MECANISCHE FRITEUSE 2 KUIPEN                                ","970X890XH930/1290                                 ",-3]
["MECA-FRYER 3B-S     ","FRITEUSE MECANIQUE BERTRAND 3 POTS                          ","MECANISCHE FRITEUSE 3 KUIPEN                                ","1450X890XH930/1290                                ",-1]
["HCL/3005-S          ","HOTTE CENTRALE AVEC 10 FILTRES INOX LABY                    ","CENTRALE DAMPKAP MET 10 INOX LABYRINTFIL                    ","3000X2000X500                                     ",1]
["HSL/11005-N         ","HOTTE MURALE ECONOMIQUE 1100                                ","STANDAARD  MUURDAMPKAP 1100                                 ","1000X1100X540                                     ",-1]
["HSL/11004-N         ","HOTTE MURALE RECONOMIQUE 1100                               ","STANDAARD  MUURDAMPKAP 1100                                 ","1000X1100X400                                     ",-1]
["HSL/11204-N         ","HOTTE MURALE RECONOMIQUE 1100                               ","STANDAARD  MUURDAMPKAP 1100                                 ","1200X1100X400                                     ",-1]
["HSL/12004-N         ","HOTTE MURALE RECONOMIQUE 1100                               ","STANDAARD  MUURDAMPKAP 1100                                 ","2000X1100X400                                     ",-1]
["HSL/12205-N         ","HOTTE MURALE RECONOMIQUE 1100                               ","STANDAARD  MUURDAMPKAP 1100                                 ","2200X1100X540                                     ",-1]
["HSL/12504-N         ","HOTTE MURALE RECONOMIQUE 1100                               ","STANDAARD  MUURDAMPKAP 1100                                 ","2500X1100X400                                     ",-1]
["HSL/12505-N         ","HOTTE MURALE RECONOMIQUE 1100                               ","STANDAARD  MUURDAMPKAP 1100                                 ","2500X1100X540                                     ",-1]
["HSL/12705-N         ","HOTTE MURALE RECONOMIQUE 1100                               ","STANDAARD  MUURDAMPKAP 1100                                 ","2700X1100X540                                     ",-1]
["HSL/1004-S          ","HOTTE MURALE RECONOMIQUE 950                                ","STANDAARD  MUURDAMPKAP 950                                  ","1000X950X400                                      ",1]
["HSL/1005-S          ","HOTTE MURALE RECONOMIQUE 950                                ","STANDAARD  MUURDAMPKAP 950                                  ","1000X950X540                                      ",4]
["HSL/1504-P-S        ","HOTTE MURALE RECONOMIQUE 950                                ","STANDAARD  MUURDAMPKAP 950                                  ","1500X950X400                                      ",-1]
["HSL/1505-S          ","HOTTE MURALE RECONOMIQUE 950                                ","STANDAARD  MUURDAMPKAP 950                                  ","1500X950X540                                      ",1]
["HSL/2004-S          ","HOTTE MURALE RECONOMIQUE 950                                ","STANDAARD  MUURDAMPKAP 950                                  ","2000X950X400                                      ",2]
["HSL/2505-S          ","HOTTE MURALE RECONOMIQUE 950                                ","STANDAARD  MUURDAMPKAP 950                                  ","2500X950X540                                      ",1]
["HSL/4004-S          ","HOTTE MURALE RECONOMIQUE 950                                ","STANDAARD  MUURDAMPKAP 950                                  ","4000X950X400                                      ",1]
["HRL/12304-S         ","HOTTE MURALE RECTANGULAIRE 1100                             ","RECHTHOEKKIGE MUURDAMPKAP 1100                              ","2300X1100X400                                     ",1]
["HRL/1004-S          ","HOTTE MURALE RECTANGULAIRE 950                              ","RECHTHOEKKIGE MUURDAMPKAP 950                               ","1000X950X400                                      ",2]
["HRL/1005-S          ","HOTTE MURALE RECTANGULAIRE 950                              ","RECHTHOEKKIGE MUURDAMPKAP 950                               ","1000X950X540                                      ",2]
["HRL/1204-S          ","HOTTE MURALE RECTANGULAIRE 950                              ","RECHTHOEKKIGE MUURDAMPKAP 950                               ","1200X950X400                                      ",1]
["HRL/1505-S          ","HOTTE MURALE RECTANGULAIRE 950                              ","RECHTHOEKKIGE MUURDAMPKAP 950                               ","1500X950X540                                      ",2]
["HRL/2504-S          ","HOTTE MURALE RECTANGULAIRE 950                              ","RECHTHOEKKIGE MUURDAMPKAP 950                               ","2500X950X400                                      ",1]
["HRL/2505-S          ","HOTTE MURALE RECTANGULAIRE 950                              ","RECHTHOEKKIGE MUURDAMPKAP 950                               ","2500X950X540                                      ",1]
["HRL/7004-S          ","HOTTE MURALE RECTANGULAIRE 950                              ","RECHTHOEKKIGE MUURDAMPKAP 950                               ","7000X950X400                                      ",1]
["KITFILHPL/1500-S    ","KIT FILTERS POUR HOTTE HPL-HPLR 1500                        ","                                                            ","                                                  ",32]
["KITFILHPL/2000-S    ","KIT FILTERS POUR HOTTE HPL-HPLR 2000                        ","                                                            ","                                                  ",31]
["KITFILHPL/2500-S    ","KIT FILTERS POUR HOTTE HPL-HPLR 2500                        ","                                                            ","                                                  ",34]
["KITVARHPL/A-S       ","KIT VARIATEUR POUR HOTTE HPL 1000-1500                      ","                                                            ","                                                  ",7]
["KITVARHPL/B-S       ","KIT VARIATEUR POUR HOTTE HPL 2000-2500                      ","                                                            ","                                                  ",-1]
["HPL/1004-DIA-S      ","HOTTE MURALE 1000 PRETE A L'EMPLOI                          ","DAMPKAP 1000 GEBRUIKSKLARE                                  ","1000X900H460                                      ",-5]
["HPL/1004-S          ","HOTTE MURALE 1000 PRETE A L'EMPLOI                          ","DAMPKAP 1000 GEBRUIKSKLARE                                  ","1000X900H460                                      ",1]
["HPL/1504-DIA-S      ","HOTTE MURALE 1500 PRETE A L'EMPLOI                          ","DAMPKAP 1500 GEBRUIKSKLARE                                  ","1500X900H460                                      ",-3]
["HPL/1504-S          ","HOTTE MURALE 1500 PRETE A L'EMPLOI                          ","DAMPKAP 1500 GEBRUIKSKLARE                                  ","1500X900H460                                      ",2]
["HPL/2004-DIA-S      ","HOTTE MURALE 2000 PRETE A L'EMPLOI                          ","DAMPKAP 2000 GEBRUIKSKLARE                                  ","2000X900H460                                      ",-5]
["HPL/2004-S          ","HOTTE MURALE 2000 PRETE A L'EMPLOI                          ","DAMPKAP 2000 GEBRUIKSKLARE                                  ","2000X900H460                                      ",1]
["HPL/2504-DIA-S      ","HOTTE MURALE 2500 PRETE A L'EMPLOI                          ","DAMPKAP 2500 GEBRUIKSKLARE                                  ","2500X900H460                                      ",2]
["HPL/2504-S          ","HOTTE MURALE 2500 PRETE A L'EMPLOI                          ","DAMPKAP 2500 GEBRUIKSKLARE                                  ","2500X900H460                                      ",5]
["HPLR/2504-S         ","HOTTE RECTANGULAIRE 2500 PRETE A L'EMPLOI                   ","DAMPKAP 2500 GEBRUIKSKLARE                                  ","2500X900H460                                      ",2]
["POUB-SNACKECO-S     ","POUBELLE DEBARASSAGE SNACK ECO                              ","VUILBAK SNACK ECO                                           ","470H470H1200                                      ",1]
["MV-950-INOX         ","VESTIAIRE INOX 2 PORTES                                     ","KLEERKAST INOX 2 DEUREN                                     ","950X500H2000                                      ",-1]
["O3990-SEUL-S        ","KIT CHAUFFANT 1200-1400-1600                                ","COMPLETE WARMTE-KIT VOOR WARMHOUDKAST                       ","KIT                                               ",8]
["L-O3980-SEUL-10-S   ","KIT CHAUFFANT AISI304SB POUR TF 1000 X 600                  ","COMPLETE WARMTE-KIT VOOR WARMHOUDKAST                       ","                                                  ",3]
["L-O3980-SEUL-S      ","KIT CHAUFFANT AISI304SB POUR TF 12-14-16 X 600              ","COMPLETE WARMTE-KIT VOOR WARMHOUDKAST                       ","                                                  ",2]
["L-O3990-SEUL-S      ","KIT CHAUFFANT AISI304SB POUR TF 12-14-16 X 700              ","COMPLETE WARMTE-KIT VOOR WARMHOUDKAST                       ","                                                  ",5]
["O3990-GX-ESCLAVE-S  ","KIT CHAUFFANT ESCLAVE GX 1800-2000                          ","KIT CHAUFFANT ESCLAVE GX 1800-2000                          ","                                                  ",2]
["O3990-DX-MASTER-S   ","KIT CHAUFFANT MASTER DX 1800 & 2000                         ","KIT CHAUFFANT MASTER DX 1800 & 2000                         ","                                                  ",2]
["O3991-SEULPASSANT-S ","KIT CHAUFFANT PASSANT 1200-1400-1600                        ","KIT CHAUFFANT PASSANT 1200-1400-1600                        ","KIT                                               ",2]
["O3991-GX-ESCLAV-PA-S","KIT CHAUFFANT PASSANT ESCLAVE GX 1800-2000                  ","KIT CHAUFFANT PASSANT ESCLAVE GX 1800-2000                  ","                                                  ",3]
["L-O3991-GX-ESCL-PA-S","KIT CHAUFFANT PASSANT ESCLAVE GX 1800-2000 AISI304SB        ","KIT CHAUFFANT PASSANT ESCLAVE GX 1800-2000 AISI304SB        ","                                                  ",2]
["O3991-DX-MASTER-PA-S","KIT CHAUFFANT PASSANT MASTER DX 1800 & 2000                 ","KIT CHAUFFANT PASSANT MASTER DX 1800 & 2000                 ","KIT                                               ",5]
["L-O3991-DX-MAS-PA-S ","KIT CHAUFFANT PASSANT MASTER DX 1800 & 2000 AISI304SB       ","KIT CHAUFFANT PASSANT MASTER DX 1800 & 2000 AISI304SB       ","KIT                                               ",1]
["ASIAOPTION96        ","CAISSON AVANT AMOVIBLE POUR FEUX CHINOIS                    ","AFNEEMBAAR VOORPANEEL VOOR CHINESE FORNUIS                  ","                                                  ",-2]
["ASIAOPTION89-C      ","COMMANDE ROBINET EAU FACE AVANT                             ","CONTROLA KRAANWATER - VOORZIJDE                             ","OPTION                                            ",-3]
["KITPIEDSALADETTE-P-S","KIT DE 4 PIEDS REGLABLES POUR SALADETTE                     ","KIT 4 REGELBAAR POTEN VOOR SALADETTE                        ","40X40XH180                                        ",-10]
["KIT4ROUE/CD2-3      ","KIT DE 4 ROUES CHARIOTS CD2-3  (2 AVEC FREINS)              ","KIT 4 WIELEN RVS KARREN CD2-3 (2 MET REM)                   ","Ø 100                                             ",-1]
["KIT4ROUE100-P-S     ","KIT DE 4 ROUES SYN Ø 100 (2 AVEC FREINS)                    ","WIELEN KIT 4x Ø 100 (2 MET REM)                             ","Ø 100                                             ",-1]
["ASIAOPTION10        ","PIETEMENT OUVERT EN TUBE CARRE                              ","OPEN ONDERSTEL IN VIERKANTE BUIS                            ","                                                  ",-7]
["C.S.S.-B+MONTAGE    ","SERRURE PORTE BATTANTE+MONTAGE                              ","SLOT VOOR KLAPDEUREN + SLEUTEL                              ","                                                  ",-1]
["ASIAOPTION11        ","SUPPORT 6 GN1/6 POUR ASIA1                                  ","STEUN 6 GN 1/6 VOOR ASIA1                                   ","600X350                                           ",-2]
["ASIAOPTION12/DX     ","SUPPORT 8 GN1/6 DROITE POUR ASIA2                           ","RECHTER HOUDER 8 GN 1/6 VOOR ASIA2                          ","770X350                                           ",-1]
["ASIAOPTION12/DX-S   ","SUPPORT 8 GN1/6 DROITE POUR ASIA2                           ","RECHTER HOUDER 8 GN 1/6 VOOR ASIA2                          ","770X350                                           ",2]
["ASIAOPTION12/GX     ","SUPPORT 8 GN1/6 GAUCHE POUR ASIA2                           ","LINKER HOUDER 8 GN 1/6 VOOR ASIA2                           ","770X350                                           ",-1]
["ASIAOPTION86        ","SYSTEME D'EAU ARRIERE                                       ","WATERSYSTEEM VOOR                                           ","                                                  ",-2]
["PAT-KITROUE         ","KIT ROUE Ø125 POUR MEUBLE PATISSERIE                        ","KIT WIELEN Ø125 VOOR BAKKERIJ KAST                          ","125                                               ",-3]
["PAT-TF/107-S        ","MODULE PATISSERIE ARMOIRE 2 PORTES COULISS                  ","BAKKERIJ MODULE KAST MET 2 SCHUIFDEUREN                     ","1000X640 H850                                     ",-1]
["PAT-TS3/600X400-S   ","MODULE PATISSERIE BLOC 3 TIROIRS 600X400                    ","BAKKERIJ MODULE BLOC 3 LADEN 600X400                        ","500X640H850                                       ",-1]
["PAT-TOP-2007-S      ","MODULE PATISSERIE TOP 2000 INOX 15/10                       ","BAKKERIJ MODULE TOP 2000 - R.V.S. 15/10                     ","2000X700H40                                       ",-1]
["PAT-TREMIE-S        ","MODULE PATISSERIE TREMIE 125L SUR ROULETTE                  ","BAKKERIJ MODULE BLOEMCONTAINER MET WIELEN 125L              ","500X640H850                                       ",-1]
["PAT-PLATEAUGALVA-S  ","PLATEAU 600X400 GALVA                                       ","PLAAT 600X400 - GALVA                                       ","600X400H20                                        ",11]
["PAT-PLATEAUINOX-S   ","PLATEAU 600X400 INOX                                        ","PLAAT 600X400 - R.V.S.                                      ","600X400H20                                        ",2]
["PLPFOND/1200-S      ","FOND PERFORE POUR PLP 1200  (BAC 1070X310H180)              ","GEPERFOREERDE BODEM VOOR PLP 1200(BAK 1070X310H180)         ","1063X303H30                                       ",3]
["PLPFOND/1400&1600-S ","FOND PERFORE POUR PLP 14+16 (BAC 1250X310H180)              ","GEPERFOREERDE BODEM VOOR PLP14+16(BAK 1250X310H180)         ","1243X303H30                                       ",10]
["PLPFOND/1600-S      ","FOND PERFORE POUR PLP 14+16 (BAC 1450X310H180)              ","                                                            ","1443X303H30                                       ",10]
["PLPFOND/1800&2000-S ","FOND PERFORE POUR PLP 18+20 (BAC 1630X310H180)              ","GEPERFOREERDE BODEM VOOR PLP 18+20(BAK 1630X310H180)        ","1623X303H30                                       ",4]
["PL/81614R+PP/0-S    ","PLONGE 1 CUVE 1360X500H400 + PP/0                           ","SPOELTAFEL 1 BAK 1360X500H400 + PP/0                        ","1600X700H900                                      ",1]
["PL/1215D+P1/LV-S    ","PLONGE 1 CUVE 500X500X325 EG.DX + P1/LV                     ","SPOELTAFEL 1 BAK 500X500X325 VERLEK R.+P1/LV                ","1200X700H900                                      ",-1]
["PL/1416D+P1/LV-S    ","PLONGE 1 CUVE 600X500X325 EG.DX + P1/LV                     ","SPOELTAFEL 1 BAK 600X500X325 VERL.RX + P1/LV                ","1400X700H900                                      ",-1]
["PL/1416D+PP/0-S     ","PLONGE 1 CUVE 600X500X325 EG.DX + PP/0                      ","SPOELTAFEL 1 BAK 600X500X325 VERL.RX + PP/0                 ","1400X700H900                                      ",1]
["PL/61424D+PP/1-S    ","PLONGE 2 CUVES 400X400X275 EG.DX + PP/1                     ","SPOELTAFEL 2 BAKKEN 400X400X275 VERL.RX+ PP/1               ","1400X600H900                                      ",2]
["PL/1624D+P0/LV-S    ","PLONGE 2 CUVES 400X500X275 EG.DX + P0/LV                    ","SPOELTAFEL 2 BAKKEN 400X500X275 VERL.RX+P0/LV               ","1600X700H900                                      ",1]
["PL/1624G+P0/LV-S    ","PLONGE 2 CUVES 400X500X275 EG.GX + P0/LV                    ","SPOELTAFEL 2 BAKKEN 400X500X275 VERL.LX+ P0/LV              ","1600X700H900                                      ",1]
["PL/2025+PP/0-S      ","PLONGE 2 CUVES 500X500X325 2 EG. + PP/0                     ","SPOELTAFEL 2 BAKKEN 500X500X325 2 VERL.+ PP/0               ","2000X700H900                                      ",3]
["PL/1825D+PP/0-S     ","PLONGE 2 CUVES 500X500X325 EG.DX + PP/0                     ","SPOELTAFEL 2 BAKKEN 500X500X325 VERL.R+ PP/0                ","1800X700H900                                      ",2]
["PL/1825G+P1/LV-S    ","PLONGE 2 CUVES 500X500X325 EG.GX + P1/LV                    ","SPOELTAFEL 2 BAKKEN 500X500X325 VERL.LX+ P1/LV              ","1800X700H900                                      ",1]
["PL/1426+PP/0-S      ","PLONGE 2 CUVES 600X500X325 + PP/0                           ","SPOELTAFEL 2 BAKKEN 600X500X325 + PP/0                      ","1400X700H900                                      ",1]
["PL/2426+PP/0-S      ","PLONGE 2 CUVES 600X500X325 2 EG. + PP/0                     ","SPOELTAFEL 2 BAKKEN 600X500X325 2 VERL. + PP/0              ","2400X700H900                                      ",2]
["PL/2226+PP/1-S      ","PLONGE 2 CUVES 600X500X325 2 EG. + PP/1                     ","SPOELTAFEL 2 BAKKEN 600X500X325 2 VERL. + PP/1              ","2200X700H900                                      ",2]
["PL/2026G+PP/0-S     ","PLONGE 2 CUVES 600X500X325 EG.GX + PP/0                     ","SPOELTAFEL 2 BAKKEN 600X500X325 VERL.LX+ PP/0               ","2000X700H900                                      ",1]
["PL/2026G+PP/1-S     ","PLONGE 2 CUVES 600X500X325 EG.GX + PP/1                     ","SPOELTAFEL 2 BAKKEN 600X500X325 VERL.LX+ PP/1               ","2000X700H900                                      ",1]
["PLPV/2070+PP/0-S    ","TABLE PREPARATION VIANDE & POISSON                          ","VOORBEREIDINGSTAFEL VLEES & VIS                             ","2000X700H900                                      ",1]
["STG64-S             ","STRUCTURE 6 NIV PLATEAU 600x400 & GN 1/1                    ","STRUCTUUR 6 NIV 600X400 & GN 1/1                            ","470X650H585                                       ",2]
["TCGX/2070-S         ","TABLE CHEF AVEC CUVE 400X400X300 GAUCHE                     ","CHEFTAFEL+SPOELBAK 400X400X300 LINKS                        ","2000X700H900                                      ",2]
["TT/0962             ","TABLE DE TRAVAIL AVEC 2 SOUS-TABLETTES                      ","WERKTAFEL MET 2 ONDERTABLETTEN                              ","900X600H900                                       ",-1]
["TT/0571-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","500X700H900                                       ",1]
["TT/0661-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","600X600H900                                       ",1]
["TT/0771-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","700X700H900                                       ",3]
["TT/0861-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","800X600H900                                       ",1]
["TT/0871-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","800X700H900                                       ",3]
["TT/1061-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1000X600H900                                      ",2]
["TT/1071-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1000X700H900                                      ",4]
["TT/1261-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1200X600H900                                      ",7]
["TT/1271-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1200X700H900                                      ",6]
["TT/1461-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1400X600H900                                      ",2]
["TT/1471-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1400X700H900                                      ",8]
["TT/1661-BAF-S       ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1600X600H900                                      ",3]
["TT/1661-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1600X600H900                                      ",2]
["TT/1671-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1600X700H900                                      ",6]
["TT/1751S            ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1700X500H900                                      ",1]
["TT/1861-BAF-S       ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1800X600H900                                      ",2]
["TT/1861-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1800X600H900                                      ",2]
["TT/1871-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1800X700H900                                      ",4]
["TT/1971-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","1900X700H900                                      ",3]
["TT/2061-BAF-S       ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","2000X600H900                                      ",1]
["TT/2061-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","2000X600H900                                      ",3]
["TT/2071-S           ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE                         ","WERKTAFEL MET ONDERTABLET                                   ","2000X700H900                                      ",9]
["TT/1671-BAF-S       ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE +BAF                    ","WERKTAFEL MET ONDERTABLET +BAF                              ","1600X700H900                                      ",1]
["TT/1871-BAF-S       ","TABLE DE TRAVAIL AVEC SOUS-TABLETTE +BAF                    ","WERKTAFEL MET ONDERTABLET +BAF                              ","1800X700H900                                      ",1]
["TT/1270-S           ","TABLE DE TRAVAIL SANS SOUS-TABLETTE                         ","WERKTAFEL ZONDER ONDERTABLET                                ","1200X700H900                                      ",1]
["TT/1670-S           ","TABLE DE TRAVAIL SANS SOUS-TABLETTE                         ","WERKTAFEL ZONDER ONDERTABLET                                ","1600X700H900                                      ",1]
["TT/2260-BAF-S       ","TABLE DE TRAVAIL SANS SOUS-TABLETTE                         ","WERKTAFEL ZONDER ONDERTABLET                                ","2200X600H900                                      ",1]
["TT/2260-S           ","TABLE DE TRAVAIL SANS SOUS-TABLETTE                         ","WERKTAFEL ZONDER ONDERTABLET                                ","2200X600H900                                      ",1]
["TT/2470-S           ","TABLE DE TRAVAIL SANS SOUS-TABLETTE                         ","WERKTAFEL ZONDER ONDERTABLET                                ","2400X700H900                                      ",1]
["TT/0970-BAF-S       ","TABLE DE TRAVAIL SANS SOUS-TABLETTE+BAF                     ","WERKTAFEL ZONDER ONDERTABLET+BAF                            ","900X700H900                                       ",1]
["TT/1870-VO-BAF-S    ","TABLE DE TRAVAIL SANS TI + VO DROITE + BAF                  ","WERKTAFEL ZONDER TABLET + VO RECHT  + BAF                   ","1800X700H900                                      ",1]
["TTDX/1271-S         ","TABLE TRAVAIL AVEC 1/2 SOUS-TABLETTE DRO                    ","WERKTAFEL MET 1/2 ONDERTABLET RECHTS                        ","1200X700H900                                      ",1]
["TTDX/1661-S         ","TABLE TRAVAIL AVEC 1/2 SOUS-TABLETTE DRO                    ","WERKTAFEL MET 1/2 ONDERTABLET RECHTS                        ","1600X600H900                                      ",1]
["TTDX/1671-S         ","TABLE TRAVAIL AVEC 1/2 SOUS-TABLETTE DRO                    ","WERKTAFEL MET 1/2 ONDERTABLET RECHTS                        ","1600X700H900                                      ",1]
["TTDX/1871-S         ","TABLE TRAVAIL AVEC 1/2 SOUS-TABLETTE DRO                    ","WERKTAFEL MET 1/2 ONDERTABLET RECHTS                        ","1800X700H900                                      ",1]
["TS/1-600-S          ","BLOC 1 TIROIR  POUR TABLE 600 MM.                           ","LADENBLOK - 1 LAD- VOOR TAFEL 600 MM                        ","400X570H180                                       ",2]
["TS/1-700-S          ","BLOC 1 TIROIR POUR TABLE 700 MM.                            ","LADENBLOK - 1 LAD- VOOR TAFEL 700 MM                        ","400X570H180                                       ",-2]
["TS/3-600-S          ","BLOC 3 TIROIRS  POUR TABLE 600                              ","LADENBLOK - 3 LADEN- VOOR TAFEL 600 MM                      ","400X570XH585                                      ",5]
["L-TS/3-600-S        ","BLOC 3 TIROIRS  POUR TABLE 600 AISI304SB                    ","BLOK VAN 3 LADEN VOOR TAFEL 600 MM AISI304SB                ","400X570XH585                                      ",3]
["TS/3-700-S          ","BLOC 3 TIROIRS  POUR TABLE 700                              ","LADENBLOK - 3 LADEN- VOOR TAFEL 700 MM                      ","400X570XH585                                      ",8]
[]
["IBERICA/PAV-01-C    ","BRÛLEUR PAELLA 10 kW A POSER                                ","BRANDER PAELLA OP DE GROND TE PLAATSEN 10kW                 ","623X355X230                                       ",1]
["IBERICA/PAV-02-C    ","BRÛLEUR PAELLA 27,2 kW A POSER                              ","BRANDER PAELLA OP DE GROND TE PLAATSEN 27,2kW               ","790X480H230                                       ",1]
["CD/7XGN1/1-C        ","CHARIOT A PLATEAU 7 X GN1/1                                 ","DIENSTKAR PLATEN 7XGN1/1                                    ","360X680H860                                       ",1]
["CD/7XGN2/1-C        ","CHARIOT A PLATEAU 7 X GN2/1                                 ","DIENSTKAR PLATEN 7XGN2/1                                    ","590X680H860                                       ",16]
["CD/7XPLATEAUX-C     ","CHARIOT A PLATEAU 7 X PLATEAUX 600x400                      ","DIENSTKAR PLATEN 7X PLATEAUX 600x400                        ","360X680H860                                       ",2]
["CD2/0850-C          ","CHARIOT DE SERVICE 2 NIVEAUX DEMONTABLE                     ","DIENSTKARRETJE 2 NIVEAU'S DEMONTEERBAAR                     ","800X500XH960                                      ",9]
["CD2/0960-C          ","CHARIOT DE SERVICE 2 NIVEAUX DEMONTABLE                     ","DIENSTKARRETJE 2 NIVEAU'S DEMONTEERBAAR                     ","900X600XH960                                      ",3]
["CD2/1050-C          ","CHARIOT DE SERVICE 2 NIVEAUX DEMONTABLE                     ","DIENSTKARRETJE 2 NIVEAU'S DEMONTEERBAAR                     ","1000X500XH960                                     ",11]
["CD3/0850-C          ","CHARIOT DE SERVICE 3 NIVEAUX DEMONTABLE                     ","DIENSTKARRETJE 3 NIVEAU'S DEMONTEERBAAR                     ","800X500XH960                                      ",2]
["CD3/0960-C          ","CHARIOT DE SERVICE 3 NIVEAUX DEMONTABLE                     ","DIENSTKARRETJE 3 NIVEAU'S DEMONTEERBAAR                     ","900X600XH960                                      ",5]
["CD3/1050-C          ","CHARIOT DE SERVICE 3 NIVEAUX DEMONTABLE                     ","DIENSTKARRETJE 3 NIVEAU'S DEMONTEERBAAR                     ","1000X500XH960                                     ",6]
["CD/15XGN1/1-C       ","CHARIOT DEMONTABLE 15 NIVEAUX GN1/1                         ","DEMONTEERBAAR GELEIDERSKARREN 15 NIV. GN1/1                 ","555X383H1480                                      ",5]
["CD/15XGN2/1-C       ","CHARIOT DEMONTABLE 15 NIVEAUX GN2/1                         ","DEMONTEERBAAR GELEIDERSKARREN 15 NIV. GN2/1                 ","675X588H1480                                      ",8]
["CD/15XPLATEAUX-C    ","CHARIOT DEMONTABLE 15 PLATEAUX 600X400                      ","DEMONTEERBAAR GELEIDERSKARREN  15 SPRINGVEER 600X400        ","625X458H1890                                      ",7]
["CD/20XGN1/1-C       ","CHARIOT DEMONTABLE 20 NIVEAUX GN1/1                         ","DEMONTEERBAAR GELEIDERSKARREN 20 NIV. GN1/1                 ","555X383H1850                                      ",20]
["CD/20XGN2/1-C       ","CHARIOT DEMONTABLE 20 NIVEAUX GN2/1                         ","DEMONTEERBAAR GELEIDERSKARREN 20 NIV. GN2/1                 ","675X588H1850                                      ",13]
["CD/20XPLATEAUX-C    ","CHARIOT DEMONTABLE 20 PLATEAUX 600X400                      ","DEMONTEERBAAR GELEIDERSKARREN 20 SPRINGVEER 600X400         ","625X460H1860                                      ",25]
["IBERICA/NT-450EC-C  ","DOSEUR A CHURROS ECO 4.5kG (MACHINE & MURAL)                ","CHURROS VERDELER ECO 4,5KG (MACHINE+MUURBEVESTIGING)        ","DOSEUR                                            ",-1]
["LVKE-1200D+VO-C     ","ENTREE LV 1200 DX + BAC 500X400 + VO KIT                    ","INLOOP R.1200 + BAK + AFVALGAT KIT                          ","1200X715H850                                      ",3]
["LVKE-1200D-C        ","ENTREE LV 1200 DX + BAC 500X400 KIT                         ","INLOOP R.1200 + BAK KIT                                     ","1200X715H850                                      ",1]
["LVKE-1200G+VO-C     ","ENTREE LV 1200 GX + BAC 500X400 + VO KIT                    ","INLOOP L.1200 + BAK + AFVALGAT KIT                          ","1200X715H850                                      ",4]
["LVKE-1200G-C        ","ENTREE LV 1200 GX + BAC 500X400 KIT                         ","INLOOP L.1200 + BAK KIT                                     ","1200X715H850                                      ",5]
["LVKE-1600D+VO-C     ","ENTREE LV 1600 DX + BAC 500X400 +VO KIT                     ","INLOOP R.1600 + BAK + AFVALGAT KIT                          ","1600X715H850                                      ",2]
["LVKE-1600G+VO-C     ","ENTREE LV 1600 GX + BAC 500X400 +VO KIT                     ","INLOOP L.1600 + BAK + AFVALGAT KIT                          ","1600X715H850                                      ",-2]
["IBERICA/KIT-PAV-01-P","KIT BBQ ET PLANCHA POUR PAV-01                              ","                                                            ","400X400H410                                       ",2]
["IBERICA/KIT-PAV-02-P","KIT BBQ ET PLANCHA POUR PAV-02                              ","                                                            ","700X700H410                                       ",3]
["O3998KIT            ","KIT DE 4 CLIPS INOX POUR ARMOIRE                            ","KIT DE 4 CLIPS INOX POUR ARMOIRE                            ","                                                  ",8]
["LP/33-SAVON-C       ","LAVE MAIN MURAL + DISTRIBUTEUR A SAVON                      ","HANDWASBAKJE + KRAAN + ZEEPDISPENSER                        ","330X330H500                                       ",42]
["LP/40-SAVON-C       ","LAVE MAIN MURAL + DISTRIBUTEUR A SAVON                      ","HANDWASBAKJE MET ZEEPDISPENSER                              ","400X340H595                                       ",47]
["LP/ECO1-C           ","LAVE MAIN MURAL MODELE \"ECO 1\"                              ","HANDWASBAKJE MODEL \"ECO 1\"                                  ","380X290                                           ",9]
["LP/ECO2-C           ","LAVE MAIN MURAL MODELE\"ECO 2\"                               ","HANDWASBAKJE MODEL \"ECO 2\"                                  ","400X320                                           ",13]
["LP/ECO2/AMM-C       ","LAVE MAIN MURAL MODELE\"ECO 2\"amm                            ","HANDWASBAKJE MODEL \"ECO 2\"amm                               ","330X330H190                                       ",12]
["LP/40-SAVON+ELEC-C  ","LAVE MAIN MURAL+ DITR.SAVON+ROBINET ELEC                    ","HANDWASBAK+ZEEPDISTR.+KRAAN ELECTR.OOG                      ","400X340H595                                       ",8]
["LP/COMBI-C          ","LAVE MAIN SUR MEUBLE                                        ","HANDWASBAKJE OP MEUBEL                                      ","500X600H900                                       ",1]
["LP/COMBI700-C       ","LAVE MAIN SUR MEUBLE                                        ","HANDWASBAKJE OP MEUBEL                                      ","500X700H900                                       ",-5]
["LA/50-C             ","LAVE MAIN SUR MEUBLE PORTE BATTENTE                         ","WASBEKKEN OP MEUBEL KNIEBEDIENING                           ","500X500X850                                       ",2]
["POUB-PINCESAC-C     ","PINCE SAC POUBELLE 110 LITRES INOX                          ","VUILZAK-KLEM 110L MET PEDAAL OP WIELEN                      ","570 X H970                                        ",18]
["POUB-PORTESAC-C     ","PORTE-SAC INOX POUR SAC 110 LITRES                          ","VUILZAK-HOUDER 110 L OP WIELEN                              ","Ø475X H850                                        ",19]
["POUB-PAP390-50L-C   ","POUBELLE INOX 50 LITRES AVEC PEDALE                         ","VUILBAK OP WIELEN 50 L MET PEDAAL                           ","Ø390X H600                                        ",29]
["POUB-PSP380-50L-C   ","POUBELLE INOX 50 LITRES SANS PEDALE                         ","VUILBAK OP WIELEN 50 L ZONDER PEDAAL                        ","Ø380X H605                                        ",31]
["POUB-PAP475-95L-C   ","POUBELLE INOX 95 LITRES AVEC PEDALE                         ","VUILBAK OP WIELEN 95 L MET PEDAAL                           ","Ø475X H720                                        ",9]
["POUB-PSP450-95L-C   ","POUBELLE INOX 95 LITRES SANS PEDALE                         ","VUILBAK 95 L ZONDER PEDAAL                                  ","Ø450X H685                                        ",15]
["C.S.S.-B            ","SERRURE PORTE BATTANTE                                      ","SLOT VOOR KLAPDEUREN + SLEUTEL                              ","                                                  ",88]
["C.S.S.-C            ","SERRURE POUSSOIR + CLEF                                     ","INDUWSLOT + SLEUTEL                                         ","OPTION                                            ",33]
["LVKS-1200-C         ","SORTIE LAVE VAISSELLE 1200 KIT                              ","UITLOOPTAFEL 1200 KIT                                       ","1200X575H850                                      ",8]
["LVKS-1600-C         ","SORTIE LAVE VAISSELLE 1600 KIT                              ","UITLOOPTAFEL 1600 KIT                                       ","1600X575H850                                      ",6]
["LVKS-0700-C         ","SORTIE LAVE VAISSELLE 700 KIT                               ","UITLOOPTAFEL 700 KIT                                        ","700X575H850                                       ",3]
["TREMIE-125L-C       ","TREMIE SUR ROUES 125 LITRES                                 ","ROLCONTAINER 125 LITER OP WIELEN                            ","395X610H785                                       ",51]
["TREMIE-150L-C       ","TREMIE SUR ROUES 150 LITRES                                 ","ROLCONTAINER 150 LITER OP WIELEN                            ","395X710H785                                       ",9]
["LED-42W             ","LED ECO CLASS DP 1200 TH42W 4000K IP65                      ","                                                            ","1210X70.5X70.4                                    ",81]
["LED-52W             ","LED ECO CLASS DP 1500 TH52W 4000K IP65                      ","                                                            ","1510X70.5X70.4                                    ",94]
["LED-21W             ","LED ECO CLASS DP 600 TH21W 4000K IP65                       ","                                                            ","610X70.5X70.4                                     ",83]
["LED-120-HPL         ","LED LINEAR 1200 POWER 14W/4000K (HPL)                       ","                                                            ","1200MM                                            ",108]
["LED-150-HPL         ","LED LINEAR 1500 POWER 25W/4000K (HPL)                       ","                                                            ","1500MM                                            ",83]
["LED-060-HPL         ","LED LINEAR 600 POWER 8W/4000K (HPL)                         ","                                                            ","600MM                                             ",87]
["SPOT/01             ","STARTER RT1014 R GU10 INDIGO                                ","                                                            ","68MM                                              ",10]
["TUBE FLUO/18        ","TUBE FLUO STANDARD 18 WATT.                                 ","                                                            ","                                                  ",20]
["TUBE FLUO/36        ","TUBE FLUO STANDARD 36 WATT.                                 ","                                                            ","                                                  ",45]
["TUBE FLUO/58        ","TUBE FLUO STANDARD 58 WATT                                  ","                                                            ","                                                  ",26]
["TE-ECHELLE-400-C    ","ECHELLE 400 4NIV. H1750                                     ","LADDERS 400 - 4 NIVEAUS / H1750                             ","1750X400                                          ",183]
["TE-ECHELLE-500-C    ","ECHELLE 500 4NIV. H1750                                     ","LADDERS 500 - 4 NIVEAUS / H1750                             ","1750X500                                          ",8]
["TE-1040/4-C         ","ETAGERE MODULABLE 1000X400                                  ","GEMODULEERD REK 1000X400                                    ","1000X400                                          ",44]
["TE-1050/5-C         ","ETAGERE MODULABLE 1000X500                                  ","GEMODULEERD REK 1000X500                                    ","1000X500                                          ",4]
["TE-1140/4-C         ","ETAGERE MODULABLE 1100X400                                  ","GEMODULEERD REK 1100X400                                    ","1100X400                                          ",36]
["TE-1150/5-C         ","ETAGERE MODULABLE 1100X500                                  ","GEMODULEERD REK 1100X500                                    ","1100X500                                          ",-16]
["TE-1240/4-C         ","ETAGERE MODULABLE 1200X400                                  ","GEMODULEERD REK 1200X400                                    ","1200X400                                          ",32]
["TE-1250/5-C         ","ETAGERE MODULABLE 1200X500                                  ","GEMODULEERD REK 1200X500                                    ","1200X500                                          ",32]
["TE-1340/4-C         ","ETAGERE MODULABLE 1300X400                                  ","GEMODULEERD REK 1300X400                                    ","1300X400                                          ",96]
["TE-1350/5-C         ","ETAGERE MODULABLE 1300X500                                  ","GEMODULEERD REK 1300X500                                    ","1300X500                                          ",16]
["TE-1440/4-C         ","ETAGERE MODULABLE 1400X400                                  ","GEMODULEERD REK 1400X400                                    ","1400X400                                          ",76]
["TE-1450/5-C         ","ETAGERE MODULABLE 1400X500                                  ","GEMODULEERD REK 1400X500                                    ","1400X500                                          ",4]
["TE-1540/4-C         ","ETAGERE MODULABLE 1500X400                                  ","GEMODULEERD REK 1500X400                                    ","1500X400                                          ",24]
["TE-1550/5-C         ","ETAGERE MODULABLE 1500X500                                  ","GEMODULEERD REK 1500X500                                    ","1500X500                                          ",20]
["TE-1640/4-C         ","ETAGERE MODULABLE 1600X400                                  ","GEMODULEERD REK 1600X400                                    ","1600X400                                          ",72]
["TE-1650/5-C         ","ETAGERE MODULABLE 1600X500                                  ","GEMODULEERD REK 1600X500                                    ","1600X500                                          ",24]
["TE-0740/4-C         ","ETAGERE MODULABLE 700X400                                   ","GEMODULEERD REK 700X400                                     ","700X400                                           ",112]
["TE-0750/5-C         ","ETAGERE MODULABLE 700X500                                   ","GEMODULEERD REK 700X500                                     ","700X500                                           ",12]
["TE-0840/4-C         ","ETAGERE MODULABLE 800X400                                   ","GEMODULEERD REK 800X400                                     ","800X400                                           ",64]
["TE-0850/5-C         ","ETAGERE MODULABLE 800X500                                   ","GEMODULEERD REK 800X500                                     ","800X500                                           ",28]
["TE-0940/4-C         ","ETAGERE MODULABLE 900X400                                   ","GEMODULEERD REK 900X400                                     ","900X400                                           ",12]
["TE-0950/5-C         ","ETAGERE MODULABLE 900X500                                   ","GEMODULEERD REK 900X500                                     ","900X500                                           ",16]
["TE-PE-C             ","PINS POUR ETAGERE MODULABLE                                 ","PINS VOOR GEMODULEERD REK                                   ","                                                  ",-16]
["TE-GA-C             ","RACCORD D'ANGLE POUR ETAGERE MODULABLE                      ","HOEKSTUK VOOR GEMODULEERD REK                               ","ANGLE                                             ",398]
["POUB-39L            ","CONTENEUR 39L POUR POUBTRI                                  ","                                                            ","                                                  ",-18]
["DS-A-C              ","DOSEUR SAVON AUTOMATIQUE                                    ","AUTOMATIC ZEEPDISPENSER                                     ","                                                  ",40]
["DS-M-C              ","DOSEUR SAVON MURAL                                          ","ZEEP VERDELER                                               ","                                                  ",3]
["BERFE230KIT-BOX     ","BOX POUR VARIATEUR HOTTE HPL                                ","                                                            ","158X118X77                                        ",186]
["HPRAL/01B           ","GRILLE POUR VENTILATEUR FRITEUSE                            ","                                                            ","                                                  ",27]
["BERFE1032I          ","VARIATEUR DE VITESSE ANALOGIQUE 8A                          ","SNELHEDENVARIATOR 8A                                        ","230VAC/50/60HZ/8A                                 ",-5]
["BERFE229            ","VARIATEUR DE VITESSE ANALOGIQUE INTER.ECLAIRAGE 5A          ","SNELHEDENVARIATOR + VERLICHT.SCHAKELAAR 5A                  ","230VAC/50/60HZ/5A                                 ",8]
["BERFE1052           ","VARIATEUR DE VITESSE ANALOGIQUE INTER.ECLAIRAGE 8A          ","SNELHEDENVARIATOR + VERLICHT.SCHAKELAAR 8A                  ","230VAC/50/60HZ/8A                                 ",-4]
["RCS 900-C           ","VARIATEUR DE VITESSE ELECTRONIQUE A.MAX                     ","ELEKTRONISCHE SNELHEDENVARIATOR VAN MAX                     ","220V/1 - 7.5AMP                                   ",1]
["RCS 210-C           ","VARIATEUR DE VITESSE ELECTRONIQUE A.MAX.                    ","ELEKTRONISCHE SNELHEDENVARIATOR VAN MAX.                    ","220V/1 - 12AMP                                    ",1]
["BERFE230KIT         ","VARIATEUR POUR HOTTE HPL 4.5A                               ","                                                            ","158X118X77                                        ",341]
["BERFE1031-DIVERSO   ","VARIATEUR POUR HOTTE HPL DIVERSO 4.5A                       ","                                                            ","                                                  ",19]
["REV17.5-C           ","VARIATEUR TRANSFO 1 X 220V - REV 17,5/5                     ","5 STANDENREGELAAR TRANSFO 1 X 220 V                         ","                                                  ",1]
["REV12.2-C           ","VARIATEUR TRANSFO 1 X 220V -REV 12,2/5 P                    ","REGELAAR TRANSFO 1 X 220V -REV 12,2/5 PO                    ","                                                  ",1]
["BERMCK10/8          ","VENTILATEUR BERDARE10/8 3000M3/H + CAISSON ISO              ","VENTILATOR  BERDARE10/8 3000M3/H + KIST ISO                 ","600X600X600                                       ",-1]
["BERMCK12/12         ","VENTILATEUR BERDARE12/12 4500M3/H + CAISSON ISO             ","VENTILATOR  BERDARE12/12 4500M3/H + KIST ISO                ","750X750X750                                       ",-7]
["BERMCK9/7           ","VENTILATEUR BERDARE9/7 2500M3/H + CAISSON ISO               ","VENTILATOR  BERDARE9/7 2500M3/H + KIST ISO                  ","600X600X600                                       ",-2]
["DA 7/7/14-C         ","VENTILATEUR CENTRIFUGE 1000 M3/H + BRIDE                    ","CENTRIFUGALE VENTILATOR 1000 M3/U + FLEN                    ","1500 TPM / A MAX. 1.7 / 147 WATT.4P./ 220V/1      ",3]
["DA 9/9/9-C          ","VENTILATEUR CENTRIFUGE 1500 M3/H + BRIDE                    ","CENTRIFUGALE VENTILATOR 1500 M3/U + FLEN                    ","1000 TPM / A MAX. 2.5 / 245 WATT.6P. / 220V/1     ",2]
["BERDA 7/7/1F4P      ","VENTILATEUR CENTRIFUGE 1500M3/H + BRIDE                     ","CENTRIFUGALE VENTILATOR 1500M3/U + FLEN                     ","                                                  ",6]
["DA 10/10/9-C        ","VENTILATEUR CENTRIFUGE 2500 M3/H + BRIDE                    ","CENTRIFUGALE VENTILATOR 2500 M3/H + FLEN                    ","1000 TPM / A MAX. 3.2 / 245 WATT.6P. / 220V/1     ",22]
["BERDA 9/71F4P1V     ","VENTILATEUR CENTRIFUGE 2500M3/H + BRIDE                     ","CENTRIFUGALE VENTILATOR 2500M3/U + FLEN                     ","                                                  ",6]
["DA 10/10/14-C       ","VENTILATEUR CENTRIFUGE 3000 M3/H + BRIDE                    ","CENTRIFUGALE VENTILATOR 3000 M3/U + FLEN                    ","1500 TPM / A MAX. 4.6 / 550 WATT.4P./ 220V/1      ",5]
["DA 9/9/14-C         ","VENTILATEUR CENTRIFUGE 3000 M3/H + BRIDE                    ","CENTRIFUGALE VENTILATOR 3000 M3/U + FLEN                    ","1500 TPM / A MAX. 5.1 / 550 WATT.4P./ 220V/1      ",8]
["BERDA 10/8-1F4P1V   ","VENTILATEUR CENTRIFUGE 3000M3/H + BRIDE                     ","CENTRIFUGALE VENTILATOR 3000M3/U + FLEN                     ","                                                  ",9]
["DA 12/9/9-C         ","VENTILATEUR CENTRIFUGE 4000 M3/H + BRIDE                    ","CENTRIFUGALE VENTILATOR 4000 M3/U + FLEN                    ","1000 TPM / A MAX. 6.8 / 736 WATT.6P. / 220V/1     ",5]
["BERDA 12/12-1F6P1V  ","VENTILATEUR CENTRIFUGE 4500M3/H + BRIDE                     ","CENTRIFUGALE VENTILATOR 4500M3/U + FLEN                     ","                                                  ",9]
["DDM 7/7-C           ","VENTILATEUR ERP2015 POUR HOTTE P.A.L (1000-1500)            ","                                                            ","1500M³/H                                          ",28]
["DDM 8/9T-C          ","VENTILATEUR ERP2015 POUR HOTTE P.A.L (2000-2500)            ","                                                            ","2500M³/H                                          ",1]
["BERDARE7/7          ","VENTILATEUR ERP2015 POUR HPL 1000-1500 (1500M³/H)           ","                                                            ","                                                  ",269]
["BERDARE9/9R         ","VENTILATEUR ERP2015 POUR HPL 2000-2500 (2500M³/H)           ","                                                            ","                                                  ",258]
["BERVDI2700PRO1F-C   ","VENTILATEUR HORS FLUX2700 MONO                              ","                                                            ","500x500x500                                       ",3]
["BERVDI4000PRO1F-C   ","VENTILATEUR HORS FLUX4000 MONO                              ","                                                            ","560X560X560/420W/2.4A                             ",1]
["BERVDI4000PRO3F-C   ","VENTILATEUR HORS FLUX4000 TRI                               ","                                                            ","560X560X560/420W/2.4A                             ",1]
["BERVDI6000PRO1F-C   ","VENTILATEUR HORS FLUX6000 MONO                              ","                                                            ","700X700X700/650W/3.5A                             ",2]
["BERVDI6000PRO3F-C   ","VENTILATEUR HORS FLUX6000 TRI                               ","                                                            ","700X700X700/650W/3.5A                             ",4]
["BERVDI8000PRO1F-C   ","VENTILATEUR HORS FLUX8000 MONO                              ","                                                            ","700X700X700/1000W/5.6A                            ",3]
["BERVDI8000PRO3F-C   ","VENTILATEUR HORS FLUX8000 TRI                               ","                                                            ","700X700X700/1000W/5.6A                            ",1]
["HPRAL/01A           ","VENTILATEUR SUR CADRE NOIR 230V -14W (FRIT)                 ","                                                            ","80X80X25                                          ",26]
["BP-C                ","BOUCHON ROND D. 40 MM EN INOX PL/HOTTE                      ","                                                            ","                                                  ",4900]
["CAOUTGRIS-C         ","CAOUTCHOUC PROTECTION VIDE ORDURE GRIS                      ","RUBBER RING VOOR AFVALGAT GRIJS                             ","                                                  ",-5]
["CORB/6050-C         ","CORBEILE POUR BAC                                           ","                                                            ","600X500X80                                        ",3]
["CORB/4040-C         ","CORBEILLE POUR BAC                                          ","                                                            ","400X400X80                                        ",3]
["CORB/5040-C         ","CORBEILLE POUR BAC                                          ","                                                            ","500X400X80                                        ",1]
["CORB5050-C          ","CORBEILLE POUR BAC                                          ","AFDRUIPROOSTER                                              ","500X500X80                                        ",3]
["PA/FEUX-C           ","CREPINE + BONDE DE DECHARGE POUR WOCK                       ","PILLETTA DI SCARICO ACIER + TUBO H150                       ","                                                  ",109]
["PA/K250+FILTRE-C    ","CREPINE + FILTRE BAC PROFONDEUR 250 MM                      ","ROOSTEROVERLOOPPIJP BAK DIEPTE 250 MM                       ","                                                  ",31]
["PA/K300+FILTRE-C    ","CREPINE + FILTRE BAC PROFONDEUR 300 MM                      ","ROOSTEROVERLOOPPIJP BAK DIEPTE 300 MM                       ","                                                  ",35]
["FOND/4040-C         ","FOND PERFORE 400X400 DROITE & GAUCHE                        ","                                                            ","400X400                                           ",13]
["FOND/D5040-C        ","FOND PERFORE 500X400 DROITE                                 ","                                                            ","500X400                                           ",3]
["FOND/G5040-C        ","FOND PERFORE 500X400 GAUCHE                                 ","                                                            ","500X400                                           ",2]
["FOND/5050-C         ","FOND PERFORE 500X500 DROITE & GAUCHE                        ","                                                            ","500X500                                           ",6]
["FOND/D6050-C        ","FOND PERFORE 600X500 DROITE                                 ","                                                            ","600X500                                           ",5]
["FOND/G6050-C        ","FOND PERFORE 600X500 GAUCHE                                 ","                                                            ","600X500                                           ",3]
["PA/K275-C           ","KIT DECHARGE -CREPINE+BONDE- CUVE PROF.2                    ","AFLOOPKIT DIEPTE 275 MM.                                    ","                                                  ",-7]
["PL/81614R-C         ","PLONGE 1 CUVE 1360X500H400                                  ","SPOELTAFEL 1 BAK 1360X500H400                               ","1600X700                                          ",2]
["PL/60615-C          ","PLONGE 1 CUVE 400X400X275                                   ","SPOELTAFEL 1 BAK 400X400X275                                ","600X600                                           ",7]
["PL/61214D-C         ","PLONGE 1 CUVE 400X400X275 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 400X400X275 VERLEK RX                      ","1200X600                                          ",1]
["PL/1014D-C          ","PLONGE 1 CUVE 400X500X275 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 400X500X275 VERLEK RX                      ","1000X700                                          ",3]
["PL/1014G-C          ","PLONGE 1 CUVE 400X500X275 EGOUTTOIR GX                      ","SPOELTAFEL 1 BAK 400X500X275 VERLEK LX                      ","1000X700                                          ",4]
["PL/1114G-C          ","PLONGE 1 CUVE 400X500X275 EGOUTTOIR GX                      ","SPOELTAFEL 1 BAK 400X500X275 VERLEK LX                      ","1100X700                                          ",-1]
["PL/90616-C          ","PLONGE 1 CUVE 450X600X300                                   ","SPOELTAFEL 1 BAK 450X600X300                                ","600X900                                           ",13]
["PL/0615-C           ","PLONGE 1 CUVE 500X400X275                                   ","SPOELTAFEL 1 BAK 500X400X275                                ","600X700                                           ",5]
["PL/61014D-C         ","PLONGE 1 CUVE 500X400X275 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 500X400X275 VERLEK RX                      ","1000X600                                          ",13]
["PL/61114D-C         ","PLONGE 1 CUVE 500X400X275 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 500X400X275 VERLEK RX                      ","1100X600                                          ",1]
["PL/61215D-C         ","PLONGE 1 CUVE 500X400X275 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 500X400X275 VERLEK RX                      ","1200X600                                          ",-2]
["PL/61014G-C         ","PLONGE 1 CUVE 500X400X275 EGOUTTOIR GX                      ","SPOELTAFEL 1 BAK 500X400X275 VERLEK LX                      ","1000X600                                          ",10]
["PL/61215G-C         ","PLONGE 1 CUVE 500X400X275 EGOUTTOIR GX                      ","SPOELTAFEL 1 BAK 500X400X275 VERLEK LX                      ","1200X600                                          ",13]
["PL/61414G-C         ","PLONGE 1 CUVE 500X400X275 EGOUTTOIR GX                      ","SPOELTAFEL 1 BAK 500X400X275 VERLEK L                       ","1400X600                                          ",1]
["PL/0715-C           ","PLONGE 1 CUVE 500X500X325                                   ","SPOELTAFEL 1 BAK 500X500X325                                ","700X700                                           ",-10]
["PL/60715-C          ","PLONGE 1 CUVE 500X500X325                                   ","SPOELTAFEL 1 BAK 500X500X325                                ","700X600                                           ",1]
["PL/1215D-C          ","PLONGE 1 CUVE 500X500X325 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 500X500X325 VERLEK RX                      ","1200X700                                          ",2]
["PL/61315D-C         ","PLONGE 1 CUVE 500X500X325 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 500X500X325 VERLEK RX                      ","1300X600                                          ",2]
["PL/1215G-C          ","PLONGE 1 CUVE 500X500X325 EGOUTTOIR GX                      ","SPOELT. 1 BAK 500X500X325 VERLEK LINKS                      ","1200X700                                          ",-2]
["PL/61315G-C         ","PLONGE 1 CUVE 500X500X325 EGOUTTOIR GX                      ","SPOELTAFEL 1 BAK 500X500X325 VERLEK LX                      ","1300X600                                          ",-1]
["PL/0816A-C          ","PLONGE 1 CUVE 600X500X325                                   ","SPOELTAFEL 1 BAK 600X500X325                                ","800X700                                           ",4]
["PL/1316D-C          ","PLONGE 1 CUVE 600X500X325 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 600X500X325 VERLEK RX                      ","1300X700                                          ",2]
["PL/1416D-C          ","PLONGE 1 CUVE 600X500X325 EGOUTTOIR DX                      ","SPOELTAFEL 1 BAK 600X500X325 VERLEK RX                      ","1400X700                                          ",-1]
["PL/1416G-C          ","PLONGE 1 CUVE 600X500X325 EGOUTTOIR GX                      ","SPOELTAFEL 1 BAK 600X500X325 VERLEK LX                      ","1400X700                                          ",6]
["PL/81018-C          ","PLONGE 1 CUVE 800X500X350                                   ","SPOELTAFEL 1 BAK 800X500X350                                ","1000X700                                          ",4]
["PL/81619G-C         ","PLONGE 1 CUVE 950X500X350 EGOUTTOIR GX                      ","SPOELTAFEL 1 BAK 950X500X350 VERLEK LX                      ","1600X700                                          ",2]
["PL/61414D-C         ","PLONGE 1 CUVE500X400X275 EGOUTTOIR DX                       ","SPOELTAFEL 1 BAK 500X400X275 VERLEK R                       ","1400X600                                          ",6]
["PL/61824G-C         ","PLONGE 2 CUVES   500X400X275 EGOUTTOIR G                    ","SPOELTAFEL 2 BAKKEN   500X400X275 VERLEK                    ","1800X600                                          ",2]
["PL/61424D-C         ","PLONGE 2 CUVES 400X400X275 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 400X400X275 VERLEK R                    ","1400X600                                          ",18]
["PL/61624D-C         ","PLONGE 2 CUVES 400X400X275 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 400X400X275 VERLEK R                    ","1600X600                                          ",4]
["PL/61424G-C         ","PLONGE 2 CUVES 400X400X275 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN400X400X275 VERLEK L                     ","1400X600                                          ",18]
["PL/61624G-C         ","PLONGE 2 CUVES 400X400X275 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN 400X400X275 VERLEK L                    ","1600X600                                          ",5]
["PL/1024-C           ","PLONGE 2 CUVES 400X500X275                                  ","SPOELTAFEL 2 BAKKEN 400X500X275                             ","1000X700                                          ",1]
["PL/61224-C          ","PLONGE 2 CUVES 400X500X275                                  ","SPOELTAFEL 2 BAKKEN 400X500X275                             ","1200X600                                          ",4]
["PL/1824-C           ","PLONGE 2 CUVES 400X500X275 2 EGOUTTOIRS                     ","SPOELTAFEL 2 BAKKEN 400X500X275 2 VERLEK                    ","1800X700                                          ",1]
["PL/1424D-C          ","PLONGE 2 CUVES 400X500X275 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 400X500X275 VERLEK R                    ","1400X700                                          ",-2]
["PL/1524D-C          ","PLONGE 2 CUVES 400X500X275 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 400X500X275 VERLEK R                    ","1500X700                                          ",2]
["PL/1624D-C          ","PLONGE 2 CUVES 400X500X275 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 400X500X275 VERLEK R                    ","1600X700                                          ",5]
["PL/1424G-C          ","PLONGE 2 CUVES 400X500X275 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN 400X500X275 VERLEK L                    ","1400X700                                          ",10]
["PL/1524G-C          ","PLONGE 2 CUVES 400X500X275 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN 400X500X275 VERLEK L                    ","1500X700                                          ",-1]
["PL/1624G-C          ","PLONGE 2 CUVES 400X500X275 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN 400X500X275 VERLEK L                    ","1600X700                                          ",11]
["PL/62024-C          ","PLONGE 2 CUVES 500X400X275 2 EGOUTTOIRS                     ","SPOELTAFEL 2 BAKKEN 500X400X275 2 VERLEK                    ","2000X600                                          ",2]
["PL/61624DA-C        ","PLONGE 2 CUVES 500X400X275 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 500X400X275 VERLEK R                    ","1600X600                                          ",1]
["PL/61824D-C         ","PLONGE 2 CUVES 500X400X275 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN  500X400X275 VERLEK                     ","1800X600                                          ",2]
["PL/1225-C           ","PLONGE 2 CUVES 500X500X325                                  ","SPOELTAFEL 2 BAKKEN 500X500X325                             ","1200X700                                          ",4]
["PL/2025-C           ","PLONGE 2 CUVES 500X500X325 2 EGOUTTOIRS                     ","SPOELTAFEL 2 BAKKEN 500X500X325 2 VERLEK                    ","2000X700                                          ",8]
["PL/1625D-C          ","PLONGE 2 CUVES 500X500X325 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 500X500X325 VERLEK R                    ","1600X700                                          ",2]
["PL/1825D-C          ","PLONGE 2 CUVES 500X500X325 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 500X500X325 VERLEK R                    ","1800X700                                          ",8]
["PL/61625DA-C        ","PLONGE 2 CUVES 500X500X325 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 500X500X325 VERLEK R                    ","1600X600                                          ",1]
["PL/1625G-C          ","PLONGE 2 CUVES 500X500X325 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN 500X500X325 VERLEK L                    ","1600X700                                          ",2]
["PL/1825G-C          ","PLONGE 2 CUVES 500X500X325 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN 500X500X325 VERLEK L                    ","1800X700                                          ",6]
["PL/1426-C           ","PLONGE 2 CUVES 600X500X325                                  ","SPOELTAFEL 2 BAKKEN 600X500X325                             ","1400X700                                          ",6]
["PL/2226-C           ","PLONGE 2 CUVES 600X500X325 2 EGOUTTOIRS                     ","SPOELTAFEL 2 BAKKEN 600X500X325 2 VERLEK                    ","2200X700                                          ",2]
["PL/2426-C           ","PLONGE 2 CUVES 600X500X325 2 EGOUTTOIRS                     ","SPOELTAFEL 2 BAKKEN 600X500X325 2 VERLEK                    ","2400X700                                          ",9]
["PL/2626-C           ","PLONGE 2 CUVES 600X500X325 2 EGOUTTOIRS                     ","SPOELTAFEL 2 BAKKEN 600X500X325 2 VERLEK                    ","2600X700                                          ",1]
["PL/2026D-C          ","PLONGE 2 CUVES 600X500X325 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 600X500X325 VERLEK R                    ","2000X700                                          ",5]
["PL/2126D-C          ","PLONGE 2 CUVES 600X500X325 EGOUTTOIR DX                     ","SPOELTAFEL 2 BAKKEN 600X500X325 VERLEK R                    ","2100X700                                          ",1]
["PL/1826G-C          ","PLONGE 2 CUVES 600X500X325 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN 600X500X325 VERLEK L                    ","1800X700                                          ",1]
["PL/2026G-C          ","PLONGE 2 CUVES 600X500X325 EGOUTTOIR GX                     ","SPOELTAFEL 2 BAKKEN 600X500X325 VERLEK L                    ","2000X700                                          ",12]
["PLPL/1270-C         ","PLONGE POUR LEGUMES (BAC 1070X310H180)                      ","                                                            ","1200X700                                          ",2]
["PLPL/1470-C         ","PLONGE POUR LEGUMES (BAC 1250X310H180)                      ","                                                            ","1400X700                                          ",-2]
["PLPL/1670-C         ","PLONGE POUR LEGUMES (BAC 1450X310H180)                      ","                                                            ","1600X700                                          ",2]
["PLPV/1470-C         ","PLONGE POUR VIANDE & POISSON                                ","                                                            ","1400X700                                          ",2]
["PLPV/1670-C         ","PLONGE POUR VIANDE & POISSON                                ","                                                            ","1600X700                                          ",1]
["PLPV/1870-C         ","PLONGE POUR VIANDE & POISSON                                ","                                                            ","1800X700                                          ",2]
["PLPV/2070-C         ","PLONGE POUR VIANDE & POISSON                                ","                                                            ","2000X700                                          ",1]
["PLPOLY/1200-C       ","POLYETHYLENE BLANC POUR PLP 1200                            ","                                                            ","730X230H20                                        ",7]
["PLPOLY/1400-C       ","POLYETHYLENE BLANC POUR PLP 1400                            ","                                                            ","930X230H20                                        ",1]
["PLPOLY/1600-C       ","POLYETHYLENE BLANC POUR PLP 1600                            ","                                                            ","1130X230H20                                       ",10]
["PLPOLY/1800-C       ","POLYETHYLENE BLANC POUR PLP 1800                            ","                                                            ","1330X230H20                                       ",1]
["PLPOLY/2000-C       ","POLYETHYLENE BLANC POUR PLP 2000                            ","                                                            ","1530X230H20                                       ",4]
["O5009               ","TOP ENTREE  1200  DX + BAC + PLIER + VO                     ","                                                            ","1200X700                                          ",4]
["O5008-DX (NEW)      ","TOP ENTREE  1200  DX + BAC PLIER                            ","                                                            ","1200X700                                          ",8]
["O5011               ","TOP ENTREE  1200  GX + BAC + PLIER + VO                     ","                                                            ","1200X700                                          ",2]
["O5008-GX (NEW)      ","TOP ENTREE  1200  GX + BAC PLIER                            ","                                                            ","1200X700                                          ",-2]
["O5014-DX            ","TOP ENTREE  1400  DX + BAC PLIER                            ","                                                            ","1400X700                                          ",2]
["O5014-GX (NEW)      ","TOP ENTREE  1400  GX + BAC PLIER                            ","                                                            ","1400X700                                          ",7]
["O5013               ","TOP ENTREE  1600  DX + BAC + PLIER + VO                     ","                                                            ","1600X700                                          ",7]
["O5012-DX (NEW)      ","TOP ENTREE  1600  DX + BAC PLIER                            ","                                                            ","1600X700                                          ",12]
["O5015               ","TOP ENTREE  1600  GX + BAC + PLIER + VO                     ","                                                            ","1600X700                                          ",-1]
["O5012-GX (NEW)      ","TOP ENTREE  1600  GX + BAC PLIER                            ","                                                            ","1600X700                                          ",5]
["O1740D-C            ","TOP PR TABLE CHEF + CUVE 40X40X30 DROITE                    ","TOP VOOR CHEFTAFEL +BAK 40X40X30 RECHTS                     ","1000X700                                          ",2]
["O1741D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1100X700                                          ",2]
["O1742D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1200X700                                          ",6]
["O1743D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1300X700                                          ",2]
["O1744D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1400X700                                          ",1]
["O1745D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1500X700                                          ",1]
["O1746D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1600X700                                          ",1]
["O1747D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1700X700                                          ",4]
["O1748D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1800X700                                          ",1]
["O1749D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","                                                            ","1900X700                                          ",1]
["O1750D-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 DROITE                     ","TOP CHEFTAFEL+SPOELBAK 40X40X30 RECHTS                      ","2000X700                                          ",11]
["O1740G-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 GAUCHE                     ","                                                            ","1000X700                                          ",8]
["O1741G-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 GAUCHE                     ","                                                            ","1100X700                                          ",2]
["O1742G-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 GAUCHE                     ","TOP VOOR CHEFTAFEL +BAK 40X40X30 LINKS                      ","1200X700                                          ",9]
["O1743G-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 GAUCHE                     ","                                                            ","1300X700                                          ",2]
["O1745G-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 GAUCHE                     ","                                                            ","1500X700                                          ",3]
["O1746G-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 GAUCHE                     ","TOP VOOR CHEFTAFEL BAK 40X40X30 LINKS                       ","1600X700                                          ",5]
["O1749G-C            ","TOP PR TABLE CHEF +CUVE 40X40X30 GAUCHE                     ","                                                            ","1900X700                                          ",2]
["O5002-GX (NEW)      ","TOP SORTIE 1200 GX PLIER                                    ","                                                            ","1200X700                                          ",5]
["O5003-DX (NEW)      ","TOP SORTIE 1600 DX PLIER                                    ","                                                            ","1600X700                                          ",1]
["O5003-GX (NEW)      ","TOP SORTIE 1600 GX PLIER                                    ","                                                            ","1600X700                                          ",13]
["O5000-DX (NEW)      ","TOP SORTIE 700 DX PLIER                                     ","                                                            ","700X700                                           ",2]
["O5000-GX (NEW)      ","TOP SORTIE 700 GX PLIER                                     ","                                                            ","700X700                                           ",8]
["O5000-GX-DX (NEW)   ","TOP SORTIE 700 PLIER SANS BORD ARRIERE                      ","                                                            ","700X700                                           ",5]
["PA/707E             ","DOUCHETTE + ROBINET MELANGEUR 1/4 DE TOUR MONOTROU          ","SPROEIER + KRAAN MENGKRAANGROEP 1/4 DRAAI (MONO)            ","                                                  ",5]
["PA/807E             ","DOUCHETTE + ROBINET MELANGEUR COMMANDE COUDE  MONOTROU      ","SPROEIER + KRAAN MENGKRAANGROEP ELLEBOOG (MONO)             ","                                                  ",5]
["PA/607E             ","DOUCHETTE + ROBINET MELANGEUR MONOTROU                      ","SPROEIER + KRAAN MENGKRAANGROEP (MONO)                      ","                                                  ",6]
["PA/707              ","DOUCHETTE AVEC MELANGEUR 1/4 DE TOUR MONOTROU               ","SPROEIER MET MENGKRAANGROEP 1/4 DRAAI (UITGANG MONO)        ","                                                  ",3]
["PA/807              ","DOUCHETTE AVEC MELANGEUR COMMANDE A COUDE MONOTROU          ","SPROEIER MET MENGKRAANGROEP ELLEBOOGBEDIENING  (UITGANG MONO","                                                  ",5]
["PA/607              ","DOUCHETTE AVEC MELANGEUR MONOTROU                           ","SPROEIER MET MENGKRAANGROEP (UITGANG MONO)                  ","                                                  ",7]
["ASIAOPTION06H550-C  ","GRAND ROBINET H 550                                         ","GROTE KRAAN HOOGTE 550 MM                                   ","OPTION                                            ",3]
["PA/907E             ","MINI DOUCHETTE + ROBINET MELANGEUR 1/4 DE TOUR MONOTROU     ","MINI SPROEIER + KRAAN MENGKRAANGROEP 1/4 DRAAI (MONO)       ","                                                  ",5]
["ASIAOPTION98-C      ","PEDALE POUR FEUX CHINOIS                                    ","PEDAAL VOOR CHINESE FORNUIS                                 ","OPTION                                            ",2]
["E012-C              ","ROBINET FACE AVANT POUR FEUX CHINOIS 1/2                    ","RUB INCASSO ECO DRITTO 1/2                                  ","                                                  ",197]
["ASIAOPTION08-C      ","ROBINET POUR RIDEAU D'EAU                                   ","                                                            ","300MM                                             ",224]
["PA/716              ","ROBINETTERIE MITIGEUR 1/4 DE TOUR MONOTROU                  ","MENGKRAAN 1/4 DRAAI                                         ","                                                  ",5]
["PA/816              ","ROBINETTERIE MITIGEUR COMMANDE COUDE MONOTROU               ","MENGKRAAN ELLEBOOGBEDIENING                                 ","                                                  ",2]
["PA/916              ","ROBINETTERIE MITIGEUR COMMANDE COUDE MONOTROU               ","MENGKRAAN ELLEBOOGBEDIENING                                 ","                                                  ",5]